| SX126x-Arduino 2.0.1

Data Fields
sMulticastParams Struct Reference
LoRa MAC layer implementation

`#include <LoRaMac.h>`

## Data Fields
uint32_t | Address
uint8_t | NwkSKey [16]
uint8_t | AppSKey [16]
uint32_t | DownLinkCounter
struct sMulticastParams * | Next

## Detailed Description

LoRaMAC multicast channel parameter

## Field Documentation

## ◆ Address

uint32_t sMulticastParams::Address

Address

## ◆ NwkSKey

uint8_t sMulticastParams::NwkSKey[16]

Network session key

## ◆ AppSKey

uint8_t sMulticastParams::AppSKey[16]

Application session key

## ◆ DownLinkCounter

uint32_t sMulticastParams::DownLinkCounter

Downlink counter

## ◆ Next

struct sMulticastParams* sMulticastParams::Next

Reference pointer to the next multicast channel parameters in the list

The documentation for this struct was generated from the following file:

- src/mac/LoRaMac.h