| SX126x-Arduino 2.0.1

Data Fields
FskBandwidth_t Struct Reference

## Data Fields
uint32_t | bandwidth
uint8_t | RegValue

## Detailed Description

FSK bandwidth definition

## Field Documentation

## ◆ bandwidth

uint32_t FskBandwidth_t::bandwidth

## ◆ RegValue

uint8_t FskBandwidth_t::RegValue

The documentation for this struct was generated from the following file:

- src/radio/sx126x/radio.cpp