| SX126x-Arduino 2.0.1

Data Fields
sRegionCommonCalcBackOffParams Struct Reference
Common region implementation

`#include <RegionCommon.h>`

## Data Fields
ChannelParams_t * | Channels
Band_t * | Bands
bool | LastTxIsJoinRequest
bool | Joined
bool | DutyCycleEnabled
uint8_t | Channel
TimerTime_t | ElapsedTime
TimerTime_t | TxTimeOnAir

## Field Documentation

## ◆ Channels

ChannelParams_t* sRegionCommonCalcBackOffParams::Channels

A pointer to region specific channels.

## ◆ Bands

Band_t* sRegionCommonCalcBackOffParams::Bands

A pointer to region specific bands.

## ◆ LastTxIsJoinRequest

bool sRegionCommonCalcBackOffParams::LastTxIsJoinRequest

Set to true, if the last uplink was a join request.

## ◆ Joined

bool sRegionCommonCalcBackOffParams::Joined

Set to true, if the node is joined.

## ◆ DutyCycleEnabled

bool sRegionCommonCalcBackOffParams::DutyCycleEnabled

Set to true, if the duty cycle is enabled.

## ◆ Channel

uint8_t sRegionCommonCalcBackOffParams::Channel

The current channel.

## ◆ ElapsedTime

TimerTime_t sRegionCommonCalcBackOffParams::ElapsedTime

The elapsed time since initialization.

## ◆ TxTimeOnAir

TimerTime_t sRegionCommonCalcBackOffParams::TxTimeOnAir

The time on air of the last Tx frame.

The documentation for this struct was generated from the following file:

- src/mac/region/RegionCommon.h