| SX126x-Arduino 2.0.1

Data Fields
PacketStatus_t Struct Reference

Represents the packet status for every packet type. More...

`#include <sx126x.h>`

## Data Fields
RadioPacketTypes_t | packetType
| Packet to which the packet status are referring to. More...
struct {
struct {
uint8_t RxStatus
int8_t RssiAvg
| The averaged RSSI. More...
int8_t RssiSync
| The RSSI measured on last packet. More...
uint32_t FreqError
} Gfsk
struct {
int8_t RssiPkt
| The RSSI of the last packet. More...
int8_t SnrPkt
| The SNR of the last packet. More...
int8_t SignalRssiPkt
uint32_t FreqError
} LoRa
} | Params

## Detailed Description

Represents the packet status for every packet type.

## Field Documentation

## ◆ packetType

RadioPacketTypes_t PacketStatus_t::packetType

Packet to which the packet status are referring to.

## ◆ RxStatus

uint8_t PacketStatus_t::RxStatus

## ◆ RssiAvg

int8_t PacketStatus_t::RssiAvg

The averaged RSSI.

## ◆ RssiSync

int8_t PacketStatus_t::RssiSync

The RSSI measured on last packet.

## ◆ FreqError

uint32_t PacketStatus_t::FreqError

## ◆ Gfsk

struct { ... } PacketStatus_t::Gfsk

## ◆ RssiPkt

int8_t PacketStatus_t::RssiPkt

The RSSI of the last packet.

## ◆ SnrPkt

int8_t PacketStatus_t::SnrPkt

The SNR of the last packet.

## ◆ SignalRssiPkt

int8_t PacketStatus_t::SignalRssiPkt

## ◆ LoRa

struct { ... } PacketStatus_t::LoRa

## ◆ Params

struct { ... } PacketStatus_t::Params

The documentation for this struct was generated from the following file:

- src/radio/sx126x/sx126x.h