| SX126x-Arduino 2.0.1

Data Fields
sChannelParams Struct Reference
LoRa MAC layer implementation

`#include <LoRaMac.h>`

## Data Fields
uint32_t | Frequency
uint32_t | Rx1Frequency
DrRange_t | DrRange
uint8_t | Band

## Detailed Description

LoRaMAC channel definition

## Field Documentation

## ◆ Frequency

uint32_t sChannelParams::Frequency

Frequency in Hz

## ◆ Rx1Frequency

uint32_t sChannelParams::Rx1Frequency

Alternative frequency for RX window 1

## ◆ DrRange

DrRange_t sChannelParams::DrRange

Data rate definition

## ◆ Band

uint8_t sChannelParams::Band

Band index

The documentation for this struct was generated from the following file:

- src/mac/LoRaMac.h