| SX126x-Arduino 2.0.1

Data Fields
sMlmeReq::uMlmeParam Union Reference

`#include <LoRaMac.h>`

## Data Fields
MlmeReqJoin_t | Join
MlmeReqTxCw_t | TxCw

## Detailed Description

MLME-Request parameters

## Field Documentation

## ◆ Join

MlmeReqJoin_t sMlmeReq::uMlmeParam::Join

MLME-Request parameters for a join request

## ◆ TxCw

MlmeReqTxCw_t sMlmeReq::uMlmeParam::TxCw

MLME-Request parameters for Tx continuous mode request

The documentation for this union was generated from the following file:

- src/mac/LoRaMac.h