| SX126x-Arduino 2.0.1

Data Fields
RadioError_t Union Reference

Represents the possible radio system error states. More...

`#include <sx126x.h>`

## Data Fields
struct {
uint8_t Rc64kCalib: 1
| RC 64kHz oscillator calibration failed. More...
uint8_t Rc13mCalib: 1
| RC 13MHz oscillator calibration failed. More...
uint8_t PllCalib: 1
| PLL calibration failed. More...
uint8_t AdcCalib: 1
| ADC calibration failed. More...
uint8_t ImgCalib: 1
| Image calibration failed. More...
uint8_t XoscStart: 1
| XOSC oscillator failed to start. More...
uint8_t PllLock: 1
| PLL lock failed. More...
uint8_t BuckStart: 1
| Buck converter failed to start. More...
uint8_t PaRamp: 1
| PA ramp failed. More...
uint8_t __pad0__: 7
| Reserved. More...
} | Fields
uint16_t | Value

## Detailed Description

Represents the possible radio system error states.

## Field Documentation

## ◆ Rc64kCalib

uint8_t RadioError_t::Rc64kCalib

RC 64kHz oscillator calibration failed.

## ◆ Rc13mCalib

uint8_t RadioError_t::Rc13mCalib

RC 13MHz oscillator calibration failed.

## ◆ PllCalib

uint8_t RadioError_t::PllCalib

PLL calibration failed.

## ◆ AdcCalib

uint8_t RadioError_t::AdcCalib

ADC calibration failed.

## ◆ ImgCalib

uint8_t RadioError_t::ImgCalib

Image calibration failed.

## ◆ XoscStart

uint8_t RadioError_t::XoscStart

XOSC oscillator failed to start.

## ◆ PllLock

uint8_t RadioError_t::PllLock

PLL lock failed.

## ◆ BuckStart

uint8_t RadioError_t::BuckStart

Buck converter failed to start.

## ◆ PaRamp

uint8_t RadioError_t::PaRamp

PA ramp failed.

## ◆ __pad0__

uint8_t RadioError_t::__pad0__

Reserved.

## ◆ Fields

struct { ... } RadioError_t::Fields

## ◆ Value

uint16_t RadioError_t::Value

The documentation for this union was generated from the following file:

- src/radio/sx126x/sx126x.h