| SX126x-Arduino 2.0.1

Data Fields
sLinkAdrReqParams Struct Reference
Region implementation

`#include <Region.h>`

## Data Fields
uint8_t * | Payload
uint8_t | PayloadSize
uint8_t | UplinkDwellTime
bool | AdrEnabled
int8_t | CurrentDatarate
int8_t | CurrentTxPower
uint8_t | CurrentNbRep

## Detailed Description

Parameter structure for the function RegionLinkAdrReq.

## Field Documentation

## ◆ Payload

uint8_t* sLinkAdrReqParams::Payload

Pointer to the payload which contains the MAC commands.

## ◆ PayloadSize

uint8_t sLinkAdrReqParams::PayloadSize

Size of the payload.

## ◆ UplinkDwellTime

uint8_t sLinkAdrReqParams::UplinkDwellTime

Uplink dwell time.

## ◆ AdrEnabled

bool sLinkAdrReqParams::AdrEnabled

Set to true, if ADR is enabled.

## ◆ CurrentDatarate

int8_t sLinkAdrReqParams::CurrentDatarate

The current datarate.

## ◆ CurrentTxPower

int8_t sLinkAdrReqParams::CurrentTxPower

The current TX power.

## ◆ CurrentNbRep

uint8_t sLinkAdrReqParams::CurrentNbRep

The current number of repetitions.

The documentation for this struct was generated from the following file:

- src/mac/region/Region.h