| SX126x-Arduino 2.0.1

Data Fields
sMlmeConfirm Struct Reference
LoRa MAC layer implementation

`#include <LoRaMac.h>`

## Data Fields
Mlme_t | MlmeRequest
LoRaMacEventInfoStatus_t | Status
TimerTime_t | TxTimeOnAir
uint8_t | DemodMargin
uint8_t | NbGateways
uint8_t | NbRetries

## Detailed Description

LoRaMAC MLME-Confirm primitive

## Field Documentation

## ◆ MlmeRequest

Mlme_t sMlmeConfirm::MlmeRequest

Holds the previously performed MLME-Request

## ◆ Status

LoRaMacEventInfoStatus_t sMlmeConfirm::Status

Status of the operation

## ◆ TxTimeOnAir

TimerTime_t sMlmeConfirm::TxTimeOnAir

The transmission time on air of the frame

## ◆ DemodMargin

uint8_t sMlmeConfirm::DemodMargin

Demodulation margin. Contains the link margin [dB] of the last successfully received LinkCheckReq

## ◆ NbGateways

uint8_t sMlmeConfirm::NbGateways

Number of gateways which received the last LinkCheckReq

## ◆ NbRetries

uint8_t sMlmeConfirm::NbRetries

Provides the number of retransmissions

The documentation for this struct was generated from the following file:

- src/mac/LoRaMac.h