| SX126x-Arduino 2.0.1

Macros | Functions
Region.cpp File Reference
`#include <stdbool.h>`
`#include <string.h>`
`#include <stdint.h>`
`#include "boards/mcu/timer.h"`
`#include "mac/LoRaMac.h"`
`#include "Region.h"`

## Macros
#define | AS923_IS_ACTIVE()
#define | AS923_GET_PHY_PARAM()
#define | AS923_SET_BAND_TX_DONE()
#define | AS923_INIT_DEFAULTS()
#define | AS923_VERIFY()
#define | AS923_APPLY_CF_LIST()
#define | AS923_CHAN_MASK_SET()
#define | AS923_ADR_NEXT()
#define | AS923_COMPUTE_RX_WINDOW_PARAMETERS()
#define | AS923_RX_CONFIG()
#define | AS923_TX_CONFIG()
#define | AS923_LINK_ADR_REQ()
#define | AS923_RX_PARAM_SETUP_REQ()
#define | AS923_NEW_CHANNEL_REQ()
#define | AS923_TX_PARAM_SETUP_REQ()
#define | AS923_DL_CHANNEL_REQ()
#define | AS923_ALTERNATE_DR()
#define | AS923_CALC_BACKOFF()
#define | AS923_NEXT_CHANNEL()
#define | AS923_CHANNEL_ADD()
#define | AS923_CHANNEL_REMOVE()
#define | AS923_SET_CONTINUOUS_WAVE()
#define | AS923_APPLY_DR_OFFSET()
#define | AS923_2_IS_ACTIVE()
#define | AS923_2_GET_PHY_PARAM()
#define | AS923_2_SET_BAND_TX_DONE()
#define | AS923_2_INIT_DEFAULTS()
#define | AS923_2_VERIFY()
#define | AS923_2_APPLY_CF_LIST()
#define | AS923_2_CHAN_MASK_SET()
#define | AS923_2_ADR_NEXT()
#define | AS923_2_COMPUTE_RX_WINDOW_PARAMETERS()
#define | AS923_2_RX_CONFIG()
#define | AS923_2_TX_CONFIG()
#define | AS923_2_LINK_ADR_REQ()
#define | AS923_2_RX_PARAM_SETUP_REQ()
#define | AS923_2_NEW_CHANNEL_REQ()
#define | AS923_2_TX_PARAM_SETUP_REQ()
#define | AS923_2_DL_CHANNEL_REQ()
#define | AS923_2_ALTERNATE_DR()
#define | AS923_2_CALC_BACKOFF()
#define | AS923_2_NEXT_CHANNEL()
#define | AS923_2_CHANNEL_ADD()
#define | AS923_2_CHANNEL_REMOVE()
#define | AS923_2_SET_CONTINUOUS_WAVE()
#define | AS923_2_APPLY_DR_OFFSET()
#define | AS923_3_IS_ACTIVE()
#define | AS923_3_GET_PHY_PARAM()
#define | AS923_3_SET_BAND_TX_DONE()
#define | AS923_3_INIT_DEFAULTS()
#define | AS923_3_VERIFY()
#define | AS923_3_APPLY_CF_LIST()
#define | AS923_3_CHAN_MASK_SET()
#define | AS923_3_ADR_NEXT()
#define | AS923_3_COMPUTE_RX_WINDOW_PARAMETERS()
#define | AS923_3_RX_CONFIG()
#define | AS923_3_TX_CONFIG()
#define | AS923_3_LINK_ADR_REQ()
#define | AS923_3_RX_PARAM_SETUP_REQ()
#define | AS923_3_NEW_CHANNEL_REQ()
#define | AS923_3_TX_PARAM_SETUP_REQ()
#define | AS923_3_DL_CHANNEL_REQ()
#define | AS923_3_ALTERNATE_DR()
#define | AS923_3_CALC_BACKOFF()
#define | AS923_3_NEXT_CHANNEL()
#define | AS923_3_CHANNEL_ADD()
#define | AS923_3_CHANNEL_REMOVE()
#define | AS923_3_SET_CONTINUOUS_WAVE()
#define | AS923_3_APPLY_DR_OFFSET()
#define | AS923_4_IS_ACTIVE()
#define | AS923_4_GET_PHY_PARAM()
#define | AS923_4_SET_BAND_TX_DONE()
#define | AS923_4_INIT_DEFAULTS()
#define | AS923_4_VERIFY()
#define | AS923_4_APPLY_CF_LIST()
#define | AS923_4_CHAN_MASK_SET()
#define | AS923_4_ADR_NEXT()
#define | AS923_4_COMPUTE_RX_WINDOW_PARAMETERS()
#define | AS923_4_RX_CONFIG()
#define | AS923_4_TX_CONFIG()
#define | AS923_4_LINK_ADR_REQ()
#define | AS923_4_RX_PARAM_SETUP_REQ()
#define | AS923_4_NEW_CHANNEL_REQ()
#define | AS923_4_TX_PARAM_SETUP_REQ()
#define | AS923_4_DL_CHANNEL_REQ()
#define | AS923_4_ALTERNATE_DR()
#define | AS923_4_CALC_BACKOFF()
#define | AS923_4_NEXT_CHANNEL()
#define | AS923_4_CHANNEL_ADD()
#define | AS923_4_CHANNEL_REMOVE()
#define | AS923_4_SET_CONTINUOUS_WAVE()
#define | AS923_4_APPLY_DR_OFFSET()
#define | AU915_IS_ACTIVE()
#define | AU915_GET_PHY_PARAM()
#define | AU915_SET_BAND_TX_DONE()
#define | AU915_INIT_DEFAULTS()
#define | AU915_VERIFY()
#define | AU915_APPLY_CF_LIST()
#define | AU915_CHAN_MASK_SET()
#define | AU915_ADR_NEXT()
#define | AU915_COMPUTE_RX_WINDOW_PARAMETERS()
#define | AU915_RX_CONFIG()
#define | AU915_TX_CONFIG()
#define | AU915_LINK_ADR_REQ()
#define | AU915_RX_PARAM_SETUP_REQ()
#define | AU915_NEW_CHANNEL_REQ()
#define | AU915_TX_PARAM_SETUP_REQ()
#define | AU915_DL_CHANNEL_REQ()
#define | AU915_ALTERNATE_DR()
#define | AU915_CALC_BACKOFF()
#define | AU915_NEXT_CHANNEL()
#define | AU915_CHANNEL_ADD()
#define | AU915_CHANNEL_REMOVE()
#define | AU915_SET_CONTINUOUS_WAVE()
#define | AU915_APPLY_DR_OFFSET()
#define | CN470_IS_ACTIVE()
#define | CN470_GET_PHY_PARAM()
#define | CN470_SET_BAND_TX_DONE()
#define | CN470_INIT_DEFAULTS()
#define | CN470_VERIFY()
#define | CN470_APPLY_CF_LIST()
#define | CN470_CHAN_MASK_SET()
#define | CN470_ADR_NEXT()
#define | CN470_COMPUTE_RX_WINDOW_PARAMETERS()
#define | CN470_RX_CONFIG()
#define | CN470_TX_CONFIG()
#define | CN470_LINK_ADR_REQ()
#define | CN470_RX_PARAM_SETUP_REQ()
#define | CN470_NEW_CHANNEL_REQ()
#define | CN470_TX_PARAM_SETUP_REQ()
#define | CN470_DL_CHANNEL_REQ()
#define | CN470_ALTERNATE_DR()
#define | CN470_CALC_BACKOFF()
#define | CN470_NEXT_CHANNEL()
#define | CN470_CHANNEL_ADD()
#define | CN470_CHANNEL_REMOVE()
#define | CN470_SET_CONTINUOUS_WAVE()
#define | CN470_APPLY_DR_OFFSET()
#define | CN779_IS_ACTIVE()
#define | CN779_GET_PHY_PARAM()
#define | CN779_SET_BAND_TX_DONE()
#define | CN779_INIT_DEFAULTS()
#define | CN779_VERIFY()
#define | CN779_APPLY_CF_LIST()
#define | CN779_CHAN_MASK_SET()
#define | CN779_ADR_NEXT()
#define | CN779_COMPUTE_RX_WINDOW_PARAMETERS()
#define | CN779_RX_CONFIG()
#define | CN779_TX_CONFIG()
#define | CN779_LINK_ADR_REQ()
#define | CN779_RX_PARAM_SETUP_REQ()
#define | CN779_NEW_CHANNEL_REQ()
#define | CN779_TX_PARAM_SETUP_REQ()
#define | CN779_DL_CHANNEL_REQ()
#define | CN779_ALTERNATE_DR()
#define | CN779_CALC_BACKOFF()
#define | CN779_NEXT_CHANNEL()
#define | CN779_CHANNEL_ADD()
#define | CN779_CHANNEL_REMOVE()
#define | CN779_SET_CONTINUOUS_WAVE()
#define | CN779_APPLY_DR_OFFSET()
#define | EU433_IS_ACTIVE()
#define | EU433_GET_PHY_PARAM()
#define | EU433_SET_BAND_TX_DONE()
#define | EU433_INIT_DEFAULTS()
#define | EU433_VERIFY()
#define | EU433_APPLY_CF_LIST()
#define | EU433_CHAN_MASK_SET()
#define | EU433_ADR_NEXT()
#define | EU433_COMPUTE_RX_WINDOW_PARAMETERS()
#define | EU433_RX_CONFIG()
#define | EU433_TX_CONFIG()
#define | EU433_LINK_ADR_REQ()
#define | EU433_RX_PARAM_SETUP_REQ()
#define | EU433_NEW_CHANNEL_REQ()
#define | EU433_TX_PARAM_SETUP_REQ()
#define | EU433_DL_CHANNEL_REQ()
#define | EU433_ALTERNATE_DR()
#define | EU433_CALC_BACKOFF()
#define | EU433_NEXT_CHANNEL()
#define | EU433_CHANNEL_ADD()
#define | EU433_CHANNEL_REMOVE()
#define | EU433_SET_CONTINUOUS_WAVE()
#define | EU433_APPLY_DR_OFFSET()
#define | EU868_IS_ACTIVE()
#define | EU868_GET_PHY_PARAM()
#define | EU868_SET_BAND_TX_DONE()
#define | EU868_INIT_DEFAULTS()
#define | EU868_VERIFY()
#define | EU868_APPLY_CF_LIST()
#define | EU868_CHAN_MASK_SET()
#define | EU868_ADR_NEXT()
#define | EU868_COMPUTE_RX_WINDOW_PARAMETERS()
#define | EU868_RX_CONFIG()
#define | EU868_TX_CONFIG()
#define | EU868_LINK_ADR_REQ()
#define | EU868_RX_PARAM_SETUP_REQ()
#define | EU868_NEW_CHANNEL_REQ()
#define | EU868_TX_PARAM_SETUP_REQ()
#define | EU868_DL_CHANNEL_REQ()
#define | EU868_ALTERNATE_DR()
#define | EU868_CALC_BACKOFF()
#define | EU868_NEXT_CHANNEL()
#define | EU868_CHANNEL_ADD()
#define | EU868_CHANNEL_REMOVE()
#define | EU868_SET_CONTINUOUS_WAVE()
#define | EU868_APPLY_DR_OFFSET()
#define | KR920_IS_ACTIVE()
#define | KR920_GET_PHY_PARAM()
#define | KR920_SET_BAND_TX_DONE()
#define | KR920_INIT_DEFAULTS()
#define | KR920_VERIFY()
#define | KR920_APPLY_CF_LIST()
#define | KR920_CHAN_MASK_SET()
#define | KR920_ADR_NEXT()
#define | KR920_COMPUTE_RX_WINDOW_PARAMETERS()
#define | KR920_RX_CONFIG()
#define | KR920_TX_CONFIG()
#define | KR920_LINK_ADR_REQ()
#define | KR920_RX_PARAM_SETUP_REQ()
#define | KR920_NEW_CHANNEL_REQ()
#define | KR920_TX_PARAM_SETUP_REQ()
#define | KR920_DL_CHANNEL_REQ()
#define | KR920_ALTERNATE_DR()
#define | KR920_CALC_BACKOFF()
#define | KR920_NEXT_CHANNEL()
#define | KR920_CHANNEL_ADD()
#define | KR920_CHANNEL_REMOVE()
#define | KR920_SET_CONTINUOUS_WAVE()
#define | KR920_APPLY_DR_OFFSET()
#define | IN865_IS_ACTIVE()
#define | IN865_GET_PHY_PARAM()
#define | IN865_SET_BAND_TX_DONE()
#define | IN865_INIT_DEFAULTS()
#define | IN865_VERIFY()
#define | IN865_APPLY_CF_LIST()
#define | IN865_CHAN_MASK_SET()
#define | IN865_ADR_NEXT()
#define | IN865_COMPUTE_RX_WINDOW_PARAMETERS()
#define | IN865_RX_CONFIG()
#define | IN865_TX_CONFIG()
#define | IN865_LINK_ADR_REQ()
#define | IN865_RX_PARAM_SETUP_REQ()
#define | IN865_NEW_CHANNEL_REQ()
#define | IN865_TX_PARAM_SETUP_REQ()
#define | IN865_DL_CHANNEL_REQ()
#define | IN865_ALTERNATE_DR()
#define | IN865_CALC_BACKOFF()
#define | IN865_NEXT_CHANNEL()
#define | IN865_CHANNEL_ADD()
#define | IN865_CHANNEL_REMOVE()
#define | IN865_SET_CONTINUOUS_WAVE()
#define | IN865_APPLY_DR_OFFSET()
#define | US915_IS_ACTIVE()
#define | US915_GET_PHY_PARAM()
#define | US915_SET_BAND_TX_DONE()
#define | US915_INIT_DEFAULTS()
#define | US915_VERIFY()
#define | US915_APPLY_CF_LIST()
#define | US915_CHAN_MASK_SET()
#define | US915_ADR_NEXT()
#define | US915_COMPUTE_RX_WINDOW_PARAMETERS()
#define | US915_RX_CONFIG()
#define | US915_TX_CONFIG()
#define | US915_LINK_ADR_REQ()
#define | US915_RX_PARAM_SETUP_REQ()
#define | US915_NEW_CHANNEL_REQ()
#define | US915_TX_PARAM_SETUP_REQ()
#define | US915_DL_CHANNEL_REQ()
#define | US915_ALTERNATE_DR()
#define | US915_CALC_BACKOFF()
#define | US915_NEXT_CHANNEL()
#define | US915_CHANNEL_ADD()
#define | US915_CHANNEL_REMOVE()
#define | US915_SET_CONTINUOUS_WAVE()
#define | US915_APPLY_DR_OFFSET()
#define | RU864_IS_ACTIVE()
#define | RU864_GET_PHY_PARAM()
#define | RU864_SET_BAND_TX_DONE()
#define | RU864_INIT_DEFAULTS()
#define | RU864_VERIFY()
#define | RU864_APPLY_CF_LIST()
#define | RU864_CHAN_MASK_SET()
#define | RU864_ADR_NEXT()
#define | RU864_COMPUTE_RX_WINDOW_PARAMETERS()
#define | RU864_RX_CONFIG()
#define | RU864_TX_CONFIG()
#define | RU864_LINK_ADR_REQ()
#define | RU864_RX_PARAM_SETUP_REQ()
#define | RU864_NEW_CHANNEL_REQ()
#define | RU864_TX_PARAM_SETUP_REQ()
#define | RU864_DL_CHANNEL_REQ()
#define | RU864_ALTERNATE_DR()
#define | RU864_CALC_BACKOFF()
#define | RU864_NEXT_CHANNEL()
#define | RU864_CHANNEL_ADD()
#define | RU864_CHANNEL_REMOVE()
#define | RU864_SET_CONTINUOUS_WAVE()
#define | RU864_APPLY_DR_OFFSET()

## Functions
bool | RegionIsActive (LoRaMacRegion_t region)
| The function verifies if a region is active or not. If a region is not active, it cannot be used. More...
PhyParam_t | RegionGetPhyParam (LoRaMacRegion_t region, GetPhyParams_t *getPhy)
| The function gets a value of a specific phy attribute. More...
void | RegionSetBandTxDone (LoRaMacRegion_t region, SetBandTxDoneParams_t *txDone)
| Updates the last TX done parameters of the current channel. More...
void | RegionInitDefaults (LoRaMacRegion_t region, InitType_t type)
| Initializes the channels masks and the channels. More...
bool | RegionVerify (LoRaMacRegion_t region, VerifyParams_t *verify, PhyAttribute_t phyAttribute)
| Verifies a parameter. More...
void | RegionApplyCFList (LoRaMacRegion_t region, ApplyCFListParams_t *applyCFList)
| The function parses the input buffer and sets up the channels of the CF list. More...
bool | RegionChanMaskSet (LoRaMacRegion_t region, ChanMaskSetParams_t *chanMaskSet)
| Sets a channels mask. More...
bool | RegionAdrNext (LoRaMacRegion_t region, AdrNextParams_t *adrNext, int8_t *drOut, int8_t *txPowOut, uint32_t *adrAckCounter)
| Calculates the next datarate to set, when ADR is on or off. More...
void | RegionComputeRxWindowParameters (LoRaMacRegion_t region, int8_t datarate, uint8_t minRxSymbols, uint32_t rxError, RxConfigParams_t *rxConfigParams)
bool | RegionRxConfig (LoRaMacRegion_t region, RxConfigParams_t *rxConfig, int8_t *datarate)
| Configuration of the RX windows. More...
bool | RegionTxConfig (LoRaMacRegion_t region, TxConfigParams_t *txConfig, int8_t *txPower, TimerTime_t *txTimeOnAir)
| TX configuration. More...
uint8_t | RegionLinkAdrReq (LoRaMacRegion_t region, LinkAdrReqParams_t *linkAdrReq, int8_t *drOut, int8_t *txPowOut, uint8_t *nbRepOut, uint8_t *nbBytesParsed)
| The function processes a Link ADR Request. More...
uint8_t | RegionRxParamSetupReq (LoRaMacRegion_t region, RxParamSetupReqParams_t *rxParamSetupReq)
| The function processes a RX Parameter Setup Request. More...
uint8_t | RegionNewChannelReq (LoRaMacRegion_t region, NewChannelReqParams_t *newChannelReq)
| The function processes a New Channel Request. More...
int8_t | RegionTxParamSetupReq (LoRaMacRegion_t region, TxParamSetupReqParams_t *txParamSetupReq)
| The function processes a TX ParamSetup Request. More...
uint8_t | RegionDlChannelReq (LoRaMacRegion_t region, DlChannelReqParams_t *dlChannelReq)
| The function processes a DlChannel Request. More...
int8_t | RegionAlternateDr (LoRaMacRegion_t region, AlternateDrParams_t *alternateDr)
| Alternates the datarate of the channel for the join request. More...
void | RegionCalcBackOff (LoRaMacRegion_t region, CalcBackOffParams_t *calcBackOff)
| Calculates the back-off time. More...
bool | RegionNextChannel (LoRaMacRegion_t region, NextChanParams_t *nextChanParams, uint8_t *channel, TimerTime_t *time, TimerTime_t *aggregatedTimeOff)
| Searches and set the next random available channel. More...
LoRaMacStatus_t | RegionChannelAdd (LoRaMacRegion_t region, ChannelAddParams_t *channelAdd)
| Adds a channel. More...
bool | RegionChannelsRemove (LoRaMacRegion_t region, ChannelRemoveParams_t *channelRemove)
| Removes a channel. More...
void | RegionSetContinuousWave (LoRaMacRegion_t region, ContinuousWaveParams_t *continuousWave)
| Sets the radio into continuous wave mode. More...
uint8_t | RegionApplyDrOffset (LoRaMacRegion_t region, uint8_t downlinkDwellTime, int8_t dr, int8_t drOffset)
| Computes new datarate according to the given offset. More...

## Macro Definition Documentation

## ◆ AS923_IS_ACTIVE

#define AS923_IS_ACTIVE | ( |  | ) |

## ◆ AS923_GET_PHY_PARAM

#define AS923_GET_PHY_PARAM | ( |  | ) |

## ◆ AS923_SET_BAND_TX_DONE

#define AS923_SET_BAND_TX_DONE | ( |  | ) |

## ◆ AS923_INIT_DEFAULTS

#define AS923_INIT_DEFAULTS | ( |  | ) |

## ◆ AS923_VERIFY

#define AS923_VERIFY | ( |  | ) |

## ◆ AS923_APPLY_CF_LIST

#define AS923_APPLY_CF_LIST | ( |  | ) |

## ◆ AS923_CHAN_MASK_SET

#define AS923_CHAN_MASK_SET | ( |  | ) |

## ◆ AS923_ADR_NEXT

#define AS923_ADR_NEXT | ( |  | ) |

## ◆ AS923_COMPUTE_RX_WINDOW_PARAMETERS

#define AS923_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ AS923_RX_CONFIG

#define AS923_RX_CONFIG | ( |  | ) |

## ◆ AS923_TX_CONFIG

#define AS923_TX_CONFIG | ( |  | ) |

## ◆ AS923_LINK_ADR_REQ

#define AS923_LINK_ADR_REQ | ( |  | ) |

## ◆ AS923_RX_PARAM_SETUP_REQ

#define AS923_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ AS923_NEW_CHANNEL_REQ

#define AS923_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ AS923_TX_PARAM_SETUP_REQ

#define AS923_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ AS923_DL_CHANNEL_REQ

#define AS923_DL_CHANNEL_REQ | ( |  | ) |

## ◆ AS923_ALTERNATE_DR

#define AS923_ALTERNATE_DR | ( |  | ) |

## ◆ AS923_CALC_BACKOFF

#define AS923_CALC_BACKOFF | ( |  | ) |

## ◆ AS923_NEXT_CHANNEL

#define AS923_NEXT_CHANNEL | ( |  | ) |

## ◆ AS923_CHANNEL_ADD

#define AS923_CHANNEL_ADD | ( |  | ) |

## ◆ AS923_CHANNEL_REMOVE

#define AS923_CHANNEL_REMOVE | ( |  | ) |

## ◆ AS923_SET_CONTINUOUS_WAVE

#define AS923_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ AS923_APPLY_DR_OFFSET

#define AS923_APPLY_DR_OFFSET | ( |  | ) |

## ◆ AS923_2_IS_ACTIVE

#define AS923_2_IS_ACTIVE | ( |  | ) |

## ◆ AS923_2_GET_PHY_PARAM

#define AS923_2_GET_PHY_PARAM | ( |  | ) |

## ◆ AS923_2_SET_BAND_TX_DONE

#define AS923_2_SET_BAND_TX_DONE | ( |  | ) |

## ◆ AS923_2_INIT_DEFAULTS

#define AS923_2_INIT_DEFAULTS | ( |  | ) |

## ◆ AS923_2_VERIFY

#define AS923_2_VERIFY | ( |  | ) |

## ◆ AS923_2_APPLY_CF_LIST

#define AS923_2_APPLY_CF_LIST | ( |  | ) |

## ◆ AS923_2_CHAN_MASK_SET

#define AS923_2_CHAN_MASK_SET | ( |  | ) |

## ◆ AS923_2_ADR_NEXT

#define AS923_2_ADR_NEXT | ( |  | ) |

## ◆ AS923_2_COMPUTE_RX_WINDOW_PARAMETERS

#define AS923_2_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ AS923_2_RX_CONFIG

#define AS923_2_RX_CONFIG | ( |  | ) |

## ◆ AS923_2_TX_CONFIG

#define AS923_2_TX_CONFIG | ( |  | ) |

## ◆ AS923_2_LINK_ADR_REQ

#define AS923_2_LINK_ADR_REQ | ( |  | ) |

## ◆ AS923_2_RX_PARAM_SETUP_REQ

#define AS923_2_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ AS923_2_NEW_CHANNEL_REQ

#define AS923_2_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ AS923_2_TX_PARAM_SETUP_REQ

#define AS923_2_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ AS923_2_DL_CHANNEL_REQ

#define AS923_2_DL_CHANNEL_REQ | ( |  | ) |

## ◆ AS923_2_ALTERNATE_DR

#define AS923_2_ALTERNATE_DR | ( |  | ) |

## ◆ AS923_2_CALC_BACKOFF

#define AS923_2_CALC_BACKOFF | ( |  | ) |

## ◆ AS923_2_NEXT_CHANNEL

#define AS923_2_NEXT_CHANNEL | ( |  | ) |

## ◆ AS923_2_CHANNEL_ADD

#define AS923_2_CHANNEL_ADD | ( |  | ) |

## ◆ AS923_2_CHANNEL_REMOVE

#define AS923_2_CHANNEL_REMOVE | ( |  | ) |

## ◆ AS923_2_SET_CONTINUOUS_WAVE

#define AS923_2_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ AS923_2_APPLY_DR_OFFSET

#define AS923_2_APPLY_DR_OFFSET | ( |  | ) |

## ◆ AS923_3_IS_ACTIVE

#define AS923_3_IS_ACTIVE | ( |  | ) |

## ◆ AS923_3_GET_PHY_PARAM

#define AS923_3_GET_PHY_PARAM | ( |  | ) |

## ◆ AS923_3_SET_BAND_TX_DONE

#define AS923_3_SET_BAND_TX_DONE | ( |  | ) |

## ◆ AS923_3_INIT_DEFAULTS

#define AS923_3_INIT_DEFAULTS | ( |  | ) |

## ◆ AS923_3_VERIFY

#define AS923_3_VERIFY | ( |  | ) |

## ◆ AS923_3_APPLY_CF_LIST

#define AS923_3_APPLY_CF_LIST | ( |  | ) |

## ◆ AS923_3_CHAN_MASK_SET

#define AS923_3_CHAN_MASK_SET | ( |  | ) |

## ◆ AS923_3_ADR_NEXT

#define AS923_3_ADR_NEXT | ( |  | ) |

## ◆ AS923_3_COMPUTE_RX_WINDOW_PARAMETERS

#define AS923_3_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ AS923_3_RX_CONFIG

#define AS923_3_RX_CONFIG | ( |  | ) |

## ◆ AS923_3_TX_CONFIG

#define AS923_3_TX_CONFIG | ( |  | ) |

## ◆ AS923_3_LINK_ADR_REQ

#define AS923_3_LINK_ADR_REQ | ( |  | ) |

## ◆ AS923_3_RX_PARAM_SETUP_REQ

#define AS923_3_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ AS923_3_NEW_CHANNEL_REQ

#define AS923_3_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ AS923_3_TX_PARAM_SETUP_REQ

#define AS923_3_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ AS923_3_DL_CHANNEL_REQ

#define AS923_3_DL_CHANNEL_REQ | ( |  | ) |

## ◆ AS923_3_ALTERNATE_DR

#define AS923_3_ALTERNATE_DR | ( |  | ) |

## ◆ AS923_3_CALC_BACKOFF

#define AS923_3_CALC_BACKOFF | ( |  | ) |

## ◆ AS923_3_NEXT_CHANNEL

#define AS923_3_NEXT_CHANNEL | ( |  | ) |

## ◆ AS923_3_CHANNEL_ADD

#define AS923_3_CHANNEL_ADD | ( |  | ) |

## ◆ AS923_3_CHANNEL_REMOVE

#define AS923_3_CHANNEL_REMOVE | ( |  | ) |

## ◆ AS923_3_SET_CONTINUOUS_WAVE

#define AS923_3_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ AS923_3_APPLY_DR_OFFSET

#define AS923_3_APPLY_DR_OFFSET | ( |  | ) |

## ◆ AS923_4_IS_ACTIVE

#define AS923_4_IS_ACTIVE | ( |  | ) |

## ◆ AS923_4_GET_PHY_PARAM

#define AS923_4_GET_PHY_PARAM | ( |  | ) |

## ◆ AS923_4_SET_BAND_TX_DONE

#define AS923_4_SET_BAND_TX_DONE | ( |  | ) |

## ◆ AS923_4_INIT_DEFAULTS

#define AS923_4_INIT_DEFAULTS | ( |  | ) |

## ◆ AS923_4_VERIFY

#define AS923_4_VERIFY | ( |  | ) |

## ◆ AS923_4_APPLY_CF_LIST

#define AS923_4_APPLY_CF_LIST | ( |  | ) |

## ◆ AS923_4_CHAN_MASK_SET

#define AS923_4_CHAN_MASK_SET | ( |  | ) |

## ◆ AS923_4_ADR_NEXT

#define AS923_4_ADR_NEXT | ( |  | ) |

## ◆ AS923_4_COMPUTE_RX_WINDOW_PARAMETERS

#define AS923_4_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ AS923_4_RX_CONFIG

#define AS923_4_RX_CONFIG | ( |  | ) |

## ◆ AS923_4_TX_CONFIG

#define AS923_4_TX_CONFIG | ( |  | ) |

## ◆ AS923_4_LINK_ADR_REQ

#define AS923_4_LINK_ADR_REQ | ( |  | ) |

## ◆ AS923_4_RX_PARAM_SETUP_REQ

#define AS923_4_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ AS923_4_NEW_CHANNEL_REQ

#define AS923_4_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ AS923_4_TX_PARAM_SETUP_REQ

#define AS923_4_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ AS923_4_DL_CHANNEL_REQ

#define AS923_4_DL_CHANNEL_REQ | ( |  | ) |

## ◆ AS923_4_ALTERNATE_DR

#define AS923_4_ALTERNATE_DR | ( |  | ) |

## ◆ AS923_4_CALC_BACKOFF

#define AS923_4_CALC_BACKOFF | ( |  | ) |

## ◆ AS923_4_NEXT_CHANNEL

#define AS923_4_NEXT_CHANNEL | ( |  | ) |

## ◆ AS923_4_CHANNEL_ADD

#define AS923_4_CHANNEL_ADD | ( |  | ) |

## ◆ AS923_4_CHANNEL_REMOVE

#define AS923_4_CHANNEL_REMOVE | ( |  | ) |

## ◆ AS923_4_SET_CONTINUOUS_WAVE

#define AS923_4_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ AS923_4_APPLY_DR_OFFSET

#define AS923_4_APPLY_DR_OFFSET | ( |  | ) |

## ◆ AU915_IS_ACTIVE

#define AU915_IS_ACTIVE | ( |  | ) |

## ◆ AU915_GET_PHY_PARAM

#define AU915_GET_PHY_PARAM | ( |  | ) |

## ◆ AU915_SET_BAND_TX_DONE

#define AU915_SET_BAND_TX_DONE | ( |  | ) |

## ◆ AU915_INIT_DEFAULTS

#define AU915_INIT_DEFAULTS | ( |  | ) |

## ◆ AU915_VERIFY

#define AU915_VERIFY | ( |  | ) |

## ◆ AU915_APPLY_CF_LIST

#define AU915_APPLY_CF_LIST | ( |  | ) |

## ◆ AU915_CHAN_MASK_SET

#define AU915_CHAN_MASK_SET | ( |  | ) |

## ◆ AU915_ADR_NEXT

#define AU915_ADR_NEXT | ( |  | ) |

## ◆ AU915_COMPUTE_RX_WINDOW_PARAMETERS

#define AU915_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ AU915_RX_CONFIG

#define AU915_RX_CONFIG | ( |  | ) |

## ◆ AU915_TX_CONFIG

#define AU915_TX_CONFIG | ( |  | ) |

## ◆ AU915_LINK_ADR_REQ

#define AU915_LINK_ADR_REQ | ( |  | ) |

## ◆ AU915_RX_PARAM_SETUP_REQ

#define AU915_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ AU915_NEW_CHANNEL_REQ

#define AU915_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ AU915_TX_PARAM_SETUP_REQ

#define AU915_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ AU915_DL_CHANNEL_REQ

#define AU915_DL_CHANNEL_REQ | ( |  | ) |

## ◆ AU915_ALTERNATE_DR

#define AU915_ALTERNATE_DR | ( |  | ) |

## ◆ AU915_CALC_BACKOFF

#define AU915_CALC_BACKOFF | ( |  | ) |

## ◆ AU915_NEXT_CHANNEL

#define AU915_NEXT_CHANNEL | ( |  | ) |

## ◆ AU915_CHANNEL_ADD

#define AU915_CHANNEL_ADD | ( |  | ) |

## ◆ AU915_CHANNEL_REMOVE

#define AU915_CHANNEL_REMOVE | ( |  | ) |

## ◆ AU915_SET_CONTINUOUS_WAVE

#define AU915_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ AU915_APPLY_DR_OFFSET

#define AU915_APPLY_DR_OFFSET | ( |  | ) |

## ◆ CN470_IS_ACTIVE

#define CN470_IS_ACTIVE | ( |  | ) |

## ◆ CN470_GET_PHY_PARAM

#define CN470_GET_PHY_PARAM | ( |  | ) |

## ◆ CN470_SET_BAND_TX_DONE

#define CN470_SET_BAND_TX_DONE | ( |  | ) |

## ◆ CN470_INIT_DEFAULTS

#define CN470_INIT_DEFAULTS | ( |  | ) |

## ◆ CN470_VERIFY

#define CN470_VERIFY | ( |  | ) |

## ◆ CN470_APPLY_CF_LIST

#define CN470_APPLY_CF_LIST | ( |  | ) |

## ◆ CN470_CHAN_MASK_SET

#define CN470_CHAN_MASK_SET | ( |  | ) |

## ◆ CN470_ADR_NEXT

#define CN470_ADR_NEXT | ( |  | ) |

## ◆ CN470_COMPUTE_RX_WINDOW_PARAMETERS

#define CN470_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ CN470_RX_CONFIG

#define CN470_RX_CONFIG | ( |  | ) |

## ◆ CN470_TX_CONFIG

#define CN470_TX_CONFIG | ( |  | ) |

## ◆ CN470_LINK_ADR_REQ

#define CN470_LINK_ADR_REQ | ( |  | ) |

## ◆ CN470_RX_PARAM_SETUP_REQ

#define CN470_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ CN470_NEW_CHANNEL_REQ

#define CN470_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ CN470_TX_PARAM_SETUP_REQ

#define CN470_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ CN470_DL_CHANNEL_REQ

#define CN470_DL_CHANNEL_REQ | ( |  | ) |

## ◆ CN470_ALTERNATE_DR

#define CN470_ALTERNATE_DR | ( |  | ) |

## ◆ CN470_CALC_BACKOFF

#define CN470_CALC_BACKOFF | ( |  | ) |

## ◆ CN470_NEXT_CHANNEL

#define CN470_NEXT_CHANNEL | ( |  | ) |

## ◆ CN470_CHANNEL_ADD

#define CN470_CHANNEL_ADD | ( |  | ) |

## ◆ CN470_CHANNEL_REMOVE

#define CN470_CHANNEL_REMOVE | ( |  | ) |

## ◆ CN470_SET_CONTINUOUS_WAVE

#define CN470_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ CN470_APPLY_DR_OFFSET

#define CN470_APPLY_DR_OFFSET | ( |  | ) |

## ◆ CN779_IS_ACTIVE

#define CN779_IS_ACTIVE | ( |  | ) |

## ◆ CN779_GET_PHY_PARAM

#define CN779_GET_PHY_PARAM | ( |  | ) |

## ◆ CN779_SET_BAND_TX_DONE

#define CN779_SET_BAND_TX_DONE | ( |  | ) |

## ◆ CN779_INIT_DEFAULTS

#define CN779_INIT_DEFAULTS | ( |  | ) |

## ◆ CN779_VERIFY

#define CN779_VERIFY | ( |  | ) |

## ◆ CN779_APPLY_CF_LIST

#define CN779_APPLY_CF_LIST | ( |  | ) |

## ◆ CN779_CHAN_MASK_SET

#define CN779_CHAN_MASK_SET | ( |  | ) |

## ◆ CN779_ADR_NEXT

#define CN779_ADR_NEXT | ( |  | ) |

## ◆ CN779_COMPUTE_RX_WINDOW_PARAMETERS

#define CN779_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ CN779_RX_CONFIG

#define CN779_RX_CONFIG | ( |  | ) |

## ◆ CN779_TX_CONFIG

#define CN779_TX_CONFIG | ( |  | ) |

## ◆ CN779_LINK_ADR_REQ

#define CN779_LINK_ADR_REQ | ( |  | ) |

## ◆ CN779_RX_PARAM_SETUP_REQ

#define CN779_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ CN779_NEW_CHANNEL_REQ

#define CN779_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ CN779_TX_PARAM_SETUP_REQ

#define CN779_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ CN779_DL_CHANNEL_REQ

#define CN779_DL_CHANNEL_REQ | ( |  | ) |

## ◆ CN779_ALTERNATE_DR

#define CN779_ALTERNATE_DR | ( |  | ) |

## ◆ CN779_CALC_BACKOFF

#define CN779_CALC_BACKOFF | ( |  | ) |

## ◆ CN779_NEXT_CHANNEL

#define CN779_NEXT_CHANNEL | ( |  | ) |

## ◆ CN779_CHANNEL_ADD

#define CN779_CHANNEL_ADD | ( |  | ) |

## ◆ CN779_CHANNEL_REMOVE

#define CN779_CHANNEL_REMOVE | ( |  | ) |

## ◆ CN779_SET_CONTINUOUS_WAVE

#define CN779_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ CN779_APPLY_DR_OFFSET

#define CN779_APPLY_DR_OFFSET | ( |  | ) |

## ◆ EU433_IS_ACTIVE

#define EU433_IS_ACTIVE | ( |  | ) |

## ◆ EU433_GET_PHY_PARAM

#define EU433_GET_PHY_PARAM | ( |  | ) |

## ◆ EU433_SET_BAND_TX_DONE

#define EU433_SET_BAND_TX_DONE | ( |  | ) |

## ◆ EU433_INIT_DEFAULTS

#define EU433_INIT_DEFAULTS | ( |  | ) |

## ◆ EU433_VERIFY

#define EU433_VERIFY | ( |  | ) |

## ◆ EU433_APPLY_CF_LIST

#define EU433_APPLY_CF_LIST | ( |  | ) |

## ◆ EU433_CHAN_MASK_SET

#define EU433_CHAN_MASK_SET | ( |  | ) |

## ◆ EU433_ADR_NEXT

#define EU433_ADR_NEXT | ( |  | ) |

## ◆ EU433_COMPUTE_RX_WINDOW_PARAMETERS

#define EU433_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ EU433_RX_CONFIG

#define EU433_RX_CONFIG | ( |  | ) |

## ◆ EU433_TX_CONFIG

#define EU433_TX_CONFIG | ( |  | ) |

## ◆ EU433_LINK_ADR_REQ

#define EU433_LINK_ADR_REQ | ( |  | ) |

## ◆ EU433_RX_PARAM_SETUP_REQ

#define EU433_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ EU433_NEW_CHANNEL_REQ

#define EU433_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ EU433_TX_PARAM_SETUP_REQ

#define EU433_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ EU433_DL_CHANNEL_REQ

#define EU433_DL_CHANNEL_REQ | ( |  | ) |

## ◆ EU433_ALTERNATE_DR

#define EU433_ALTERNATE_DR | ( |  | ) |

## ◆ EU433_CALC_BACKOFF

#define EU433_CALC_BACKOFF | ( |  | ) |

## ◆ EU433_NEXT_CHANNEL

#define EU433_NEXT_CHANNEL | ( |  | ) |

## ◆ EU433_CHANNEL_ADD

#define EU433_CHANNEL_ADD | ( |  | ) |

## ◆ EU433_CHANNEL_REMOVE

#define EU433_CHANNEL_REMOVE | ( |  | ) |

## ◆ EU433_SET_CONTINUOUS_WAVE

#define EU433_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ EU433_APPLY_DR_OFFSET

#define EU433_APPLY_DR_OFFSET | ( |  | ) |

## ◆ EU868_IS_ACTIVE

#define EU868_IS_ACTIVE | ( |  | ) |

## ◆ EU868_GET_PHY_PARAM

#define EU868_GET_PHY_PARAM | ( |  | ) |

## ◆ EU868_SET_BAND_TX_DONE

#define EU868_SET_BAND_TX_DONE | ( |  | ) |

## ◆ EU868_INIT_DEFAULTS

#define EU868_INIT_DEFAULTS | ( |  | ) |

## ◆ EU868_VERIFY

#define EU868_VERIFY | ( |  | ) |

## ◆ EU868_APPLY_CF_LIST

#define EU868_APPLY_CF_LIST | ( |  | ) |

## ◆ EU868_CHAN_MASK_SET

#define EU868_CHAN_MASK_SET | ( |  | ) |

## ◆ EU868_ADR_NEXT

#define EU868_ADR_NEXT | ( |  | ) |

## ◆ EU868_COMPUTE_RX_WINDOW_PARAMETERS

#define EU868_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ EU868_RX_CONFIG

#define EU868_RX_CONFIG | ( |  | ) |

## ◆ EU868_TX_CONFIG

#define EU868_TX_CONFIG | ( |  | ) |

## ◆ EU868_LINK_ADR_REQ

#define EU868_LINK_ADR_REQ | ( |  | ) |

## ◆ EU868_RX_PARAM_SETUP_REQ

#define EU868_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ EU868_NEW_CHANNEL_REQ

#define EU868_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ EU868_TX_PARAM_SETUP_REQ

#define EU868_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ EU868_DL_CHANNEL_REQ

#define EU868_DL_CHANNEL_REQ | ( |  | ) |

## ◆ EU868_ALTERNATE_DR

#define EU868_ALTERNATE_DR | ( |  | ) |

## ◆ EU868_CALC_BACKOFF

#define EU868_CALC_BACKOFF | ( |  | ) |

## ◆ EU868_NEXT_CHANNEL

#define EU868_NEXT_CHANNEL | ( |  | ) |

## ◆ EU868_CHANNEL_ADD

#define EU868_CHANNEL_ADD | ( |  | ) |

## ◆ EU868_CHANNEL_REMOVE

#define EU868_CHANNEL_REMOVE | ( |  | ) |

## ◆ EU868_SET_CONTINUOUS_WAVE

#define EU868_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ EU868_APPLY_DR_OFFSET

#define EU868_APPLY_DR_OFFSET | ( |  | ) |

## ◆ KR920_IS_ACTIVE

#define KR920_IS_ACTIVE | ( |  | ) |

## ◆ KR920_GET_PHY_PARAM

#define KR920_GET_PHY_PARAM | ( |  | ) |

## ◆ KR920_SET_BAND_TX_DONE

#define KR920_SET_BAND_TX_DONE | ( |  | ) |

## ◆ KR920_INIT_DEFAULTS

#define KR920_INIT_DEFAULTS | ( |  | ) |

## ◆ KR920_VERIFY

#define KR920_VERIFY | ( |  | ) |

## ◆ KR920_APPLY_CF_LIST

#define KR920_APPLY_CF_LIST | ( |  | ) |

## ◆ KR920_CHAN_MASK_SET

#define KR920_CHAN_MASK_SET | ( |  | ) |

## ◆ KR920_ADR_NEXT

#define KR920_ADR_NEXT | ( |  | ) |

## ◆ KR920_COMPUTE_RX_WINDOW_PARAMETERS

#define KR920_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ KR920_RX_CONFIG

#define KR920_RX_CONFIG | ( |  | ) |

## ◆ KR920_TX_CONFIG

#define KR920_TX_CONFIG | ( |  | ) |

## ◆ KR920_LINK_ADR_REQ

#define KR920_LINK_ADR_REQ | ( |  | ) |

## ◆ KR920_RX_PARAM_SETUP_REQ

#define KR920_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ KR920_NEW_CHANNEL_REQ

#define KR920_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ KR920_TX_PARAM_SETUP_REQ

#define KR920_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ KR920_DL_CHANNEL_REQ

#define KR920_DL_CHANNEL_REQ | ( |  | ) |

## ◆ KR920_ALTERNATE_DR

#define KR920_ALTERNATE_DR | ( |  | ) |

## ◆ KR920_CALC_BACKOFF

#define KR920_CALC_BACKOFF | ( |  | ) |

## ◆ KR920_NEXT_CHANNEL

#define KR920_NEXT_CHANNEL | ( |  | ) |

## ◆ KR920_CHANNEL_ADD

#define KR920_CHANNEL_ADD | ( |  | ) |

## ◆ KR920_CHANNEL_REMOVE

#define KR920_CHANNEL_REMOVE | ( |  | ) |

## ◆ KR920_SET_CONTINUOUS_WAVE

#define KR920_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ KR920_APPLY_DR_OFFSET

#define KR920_APPLY_DR_OFFSET | ( |  | ) |

## ◆ IN865_IS_ACTIVE

#define IN865_IS_ACTIVE | ( |  | ) |

## ◆ IN865_GET_PHY_PARAM

#define IN865_GET_PHY_PARAM | ( |  | ) |

## ◆ IN865_SET_BAND_TX_DONE

#define IN865_SET_BAND_TX_DONE | ( |  | ) |

## ◆ IN865_INIT_DEFAULTS

#define IN865_INIT_DEFAULTS | ( |  | ) |

## ◆ IN865_VERIFY

#define IN865_VERIFY | ( |  | ) |

## ◆ IN865_APPLY_CF_LIST

#define IN865_APPLY_CF_LIST | ( |  | ) |

## ◆ IN865_CHAN_MASK_SET

#define IN865_CHAN_MASK_SET | ( |  | ) |

## ◆ IN865_ADR_NEXT

#define IN865_ADR_NEXT | ( |  | ) |

## ◆ IN865_COMPUTE_RX_WINDOW_PARAMETERS

#define IN865_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ IN865_RX_CONFIG

#define IN865_RX_CONFIG | ( |  | ) |

## ◆ IN865_TX_CONFIG

#define IN865_TX_CONFIG | ( |  | ) |

## ◆ IN865_LINK_ADR_REQ

#define IN865_LINK_ADR_REQ | ( |  | ) |

## ◆ IN865_RX_PARAM_SETUP_REQ

#define IN865_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ IN865_NEW_CHANNEL_REQ

#define IN865_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ IN865_TX_PARAM_SETUP_REQ

#define IN865_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ IN865_DL_CHANNEL_REQ

#define IN865_DL_CHANNEL_REQ | ( |  | ) |

## ◆ IN865_ALTERNATE_DR

#define IN865_ALTERNATE_DR | ( |  | ) |

## ◆ IN865_CALC_BACKOFF

#define IN865_CALC_BACKOFF | ( |  | ) |

## ◆ IN865_NEXT_CHANNEL

#define IN865_NEXT_CHANNEL | ( |  | ) |

## ◆ IN865_CHANNEL_ADD

#define IN865_CHANNEL_ADD | ( |  | ) |

## ◆ IN865_CHANNEL_REMOVE

#define IN865_CHANNEL_REMOVE | ( |  | ) |

## ◆ IN865_SET_CONTINUOUS_WAVE

#define IN865_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ IN865_APPLY_DR_OFFSET

#define IN865_APPLY_DR_OFFSET | ( |  | ) |

## ◆ US915_IS_ACTIVE

#define US915_IS_ACTIVE | ( |  | ) |

## ◆ US915_GET_PHY_PARAM

#define US915_GET_PHY_PARAM | ( |  | ) |

## ◆ US915_SET_BAND_TX_DONE

#define US915_SET_BAND_TX_DONE | ( |  | ) |

## ◆ US915_INIT_DEFAULTS

#define US915_INIT_DEFAULTS | ( |  | ) |

## ◆ US915_VERIFY

#define US915_VERIFY | ( |  | ) |

## ◆ US915_APPLY_CF_LIST

#define US915_APPLY_CF_LIST | ( |  | ) |

## ◆ US915_CHAN_MASK_SET

#define US915_CHAN_MASK_SET | ( |  | ) |

## ◆ US915_ADR_NEXT

#define US915_ADR_NEXT | ( |  | ) |

## ◆ US915_COMPUTE_RX_WINDOW_PARAMETERS

#define US915_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ US915_RX_CONFIG

#define US915_RX_CONFIG | ( |  | ) |

## ◆ US915_TX_CONFIG

#define US915_TX_CONFIG | ( |  | ) |

## ◆ US915_LINK_ADR_REQ

#define US915_LINK_ADR_REQ | ( |  | ) |

## ◆ US915_RX_PARAM_SETUP_REQ

#define US915_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ US915_NEW_CHANNEL_REQ

#define US915_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ US915_TX_PARAM_SETUP_REQ

#define US915_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ US915_DL_CHANNEL_REQ

#define US915_DL_CHANNEL_REQ | ( |  | ) |

## ◆ US915_ALTERNATE_DR

#define US915_ALTERNATE_DR | ( |  | ) |

## ◆ US915_CALC_BACKOFF

#define US915_CALC_BACKOFF | ( |  | ) |

## ◆ US915_NEXT_CHANNEL

#define US915_NEXT_CHANNEL | ( |  | ) |

## ◆ US915_CHANNEL_ADD

#define US915_CHANNEL_ADD | ( |  | ) |

## ◆ US915_CHANNEL_REMOVE

#define US915_CHANNEL_REMOVE | ( |  | ) |

## ◆ US915_SET_CONTINUOUS_WAVE

#define US915_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ US915_APPLY_DR_OFFSET

#define US915_APPLY_DR_OFFSET | ( |  | ) |

## ◆ RU864_IS_ACTIVE

#define RU864_IS_ACTIVE | ( |  | ) |

## ◆ RU864_GET_PHY_PARAM

#define RU864_GET_PHY_PARAM | ( |  | ) |

## ◆ RU864_SET_BAND_TX_DONE

#define RU864_SET_BAND_TX_DONE | ( |  | ) |

## ◆ RU864_INIT_DEFAULTS

#define RU864_INIT_DEFAULTS | ( |  | ) |

## ◆ RU864_VERIFY

#define RU864_VERIFY | ( |  | ) |

## ◆ RU864_APPLY_CF_LIST

#define RU864_APPLY_CF_LIST | ( |  | ) |

## ◆ RU864_CHAN_MASK_SET

#define RU864_CHAN_MASK_SET | ( |  | ) |

## ◆ RU864_ADR_NEXT

#define RU864_ADR_NEXT | ( |  | ) |

## ◆ RU864_COMPUTE_RX_WINDOW_PARAMETERS

#define RU864_COMPUTE_RX_WINDOW_PARAMETERS | ( |  | ) |

## ◆ RU864_RX_CONFIG

#define RU864_RX_CONFIG | ( |  | ) |

## ◆ RU864_TX_CONFIG

#define RU864_TX_CONFIG | ( |  | ) |

## ◆ RU864_LINK_ADR_REQ

#define RU864_LINK_ADR_REQ | ( |  | ) |

## ◆ RU864_RX_PARAM_SETUP_REQ

#define RU864_RX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ RU864_NEW_CHANNEL_REQ

#define RU864_NEW_CHANNEL_REQ | ( |  | ) |

## ◆ RU864_TX_PARAM_SETUP_REQ

#define RU864_TX_PARAM_SETUP_REQ | ( |  | ) |

## ◆ RU864_DL_CHANNEL_REQ

#define RU864_DL_CHANNEL_REQ | ( |  | ) |

## ◆ RU864_ALTERNATE_DR

#define RU864_ALTERNATE_DR | ( |  | ) |

## ◆ RU864_CALC_BACKOFF

#define RU864_CALC_BACKOFF | ( |  | ) |

## ◆ RU864_NEXT_CHANNEL

#define RU864_NEXT_CHANNEL | ( |  | ) |

## ◆ RU864_CHANNEL_ADD

#define RU864_CHANNEL_ADD | ( |  | ) |

## ◆ RU864_CHANNEL_REMOVE

#define RU864_CHANNEL_REMOVE | ( |  | ) |

## ◆ RU864_SET_CONTINUOUS_WAVE

#define RU864_SET_CONTINUOUS_WAVE | ( |  | ) |

## ◆ RU864_APPLY_DR_OFFSET

#define RU864_APPLY_DR_OFFSET | ( |  | ) |