| SX126x-Arduino 2.0.1

Data Fields
uDrRange::sFields Struct Reference

`#include <LoRaMac.h>`

## Data Fields
int8_t | Min: 4
int8_t | Max: 4

## Detailed Description

Structure to store the minimum and the maximum datarate

## Field Documentation

## ◆ Min

int8_t uDrRange::sFields::Min

Minimum data rate

LoRaWAN Regional Parameters V1.0.2rB

The allowed ranges are region specific. Please refer to DR_0 to DR_15 for details.

## ◆ Max

int8_t uDrRange::sFields::Max

Maximum data rate

LoRaWAN Regional Parameters V1.0.2rB

The allowed ranges are region specific. Please refer to DR_0 to DR_15 for details.

The documentation for this struct was generated from the following file:

- src/mac/LoRaMac.h