| SX126x-Arduino 2.0.1

Data Fields
sGetPhyParams Struct Reference
Region implementation

`#include <Region.h>`

## Data Fields
PhyAttribute_t | Attribute
int8_t | Datarate
uint8_t | UplinkDwellTime
uint8_t | DownlinkDwellTime

## Detailed Description

Parameter structure for the function RegionGetPhyParam.

## Field Documentation

## ◆ Attribute

PhyAttribute_t sGetPhyParams::Attribute

Setup the parameter to get.

## ◆ Datarate

int8_t sGetPhyParams::Datarate

Datarate. The parameter is needed for the following queries: PHY_MAX_PAYLOAD, PHY_MAX_PAYLOAD_REPEATER, PHY_NEXT_LOWER_TX_DR.

## ◆ UplinkDwellTime

uint8_t sGetPhyParams::UplinkDwellTime

Uplink dwell time. The parameter is needed for the following queries: PHY_MIN_TX_DR, PHY_MAX_PAYLOAD, PHY_MAX_PAYLOAD_REPEATER, PHY_NEXT_LOWER_TX_DR.

## ◆ DownlinkDwellTime

uint8_t sGetPhyParams::DownlinkDwellTime

Downlink dwell time. The parameter is needed for the following queries: PHY_MIN_RX_DR, PHY_MAX_PAYLOAD, PHY_MAX_PAYLOAD_REPEATER.

The documentation for this struct was generated from the following file:

- src/mac/region/Region.h