| SX126x-Arduino 2.0.1

Data Fields
sMlmeReqTxCw Struct Reference
LoRa MAC layer implementation

`#include <LoRaMac.h>`

## Data Fields
uint16_t | Timeout
uint32_t | Frequency
uint8_t | Power

## Detailed Description

LoRaMAC MLME-Request for Tx continuous wave mode

## Field Documentation

## ◆ Timeout

uint16_t sMlmeReqTxCw::Timeout

Time in seconds while the radio is kept in continuous wave mode

## ◆ Frequency

uint32_t sMlmeReqTxCw::Frequency

RF frequency to set (Only used with new way)

## ◆ Power

uint8_t sMlmeReqTxCw::Power

RF output power to set (Only used with new way)

The documentation for this struct was generated from the following file:

- src/mac/LoRaMac.h