| SX126x-Arduino 2.0.1

Data Fields
sRx2ChannelParams Struct Reference
LoRa MAC layer implementation

`#include <LoRaMac.h>`

## Data Fields
uint32_t | Frequency
uint8_t | Datarate

## Detailed Description

LoRaMAC receive window 2 channel parameters

## Field Documentation

## ◆ Frequency

uint32_t sRx2ChannelParams::Frequency

Frequency in Hz

## ◆ Datarate

uint8_t sRx2ChannelParams::Datarate

Data rate

LoRaWAN Regional Parameters V1.0.2rB

The allowed ranges are region specific. Please refer to DR_0 to DR_15 for details.

The documentation for this struct was generated from the following file:

- src/mac/LoRaMac.h