| SX126x-Arduino 2.0.1

Data Structures
Here are the data structures with brief descriptions:
[detail level 1 2]

C_AES_CMAC_CTX |
C CalibrationParams_t | Represents a calibration configuration
▼C eLoRaMacFlags_t |
C sMacFlagBits |
C eMibRequestConfirm |
C FskBandwidth_t |
C hw_config |
C lmh_app_data_t | Application Data structure
C lmh_callback_s | LoRaMac Helper Callbacks
C lmh_param_s |
C lora_aes_context |
C LoraMacHelper_ComplianceTest_s | LoRaWAN compliance tests support data
C ModulationParams_t | The type describing the modulation parameters for every packet types
C PacketParams_t | The type describing the packet parameters for every packet types
C PacketStatus_t | Represents the packet status for every packet type
C Radio_s | Radio driver definition
C RadioError_t | Represents the possible radio system error states
C RadioEvents_t | Radio driver callback functions
C RadioPublicNetwork_t |
C RadioRegisters_t | Radio registers definition
C RadioStatus_u | Structure describing the radio status
C RxCounter_t | Represents the Rx internal counters values when GFSK or LoRa packet type is used
C sAdrNextParams |
C sAlternateDrParams |
C sApplyCFListParams |
C sBand |
C sCalcBackOffParams |
C sChanMaskSetParams |
C sChannelAddParams |
C sChannelParams |
C sChannelRemoveParams |
C sContinuousWaveParams |
C sDlChannelReqParams |
C sGetPhyParams |
C SleepParams_t | Represents a sleep mode configuration
C sLinkAdrReqParams |
C sLoRaMacCallback |
C sLoRaMacParams |
C sLoRaMacPrimitives |
C sLoRaMacTxInfo |
C sMcpsConfirm |
C sMcpsIndication |
▼C sMcpsReq |
C uMcpsParam |
C sMcpsReqConfirmed |
C sMcpsReqProprietary |
C sMcpsReqUnconfirmed |
C sMlmeConfirm |
▼C sMlmeReq |
C uMlmeParam |
C sMlmeReqJoin |
C sMlmeReqTxCw |
C sMulticastParams |
C sNewChannelReqParams |
C sNextChanParams |
C sRegionCommonCalcBackOffParams |
C sRegionCommonLinkAdrParams |
C sRegionCommonLinkAdrReqVerifyParams |
C sRx2ChannelParams |
C sRxConfigParams |
C sRxParamSetupReqParams |
C sSetBandTxDoneParams |
C sTxConfigParams |
C sTxParamSetupReqParams |
C SX126x_s |
C SX126xCallbacks_t | The radio callbacks structure Holds function pointers to be called on radio interrupts
C TimerEvent_s | Timer object description
▼C uDrRange |
C sFields |
▼C uLoRaMacFrameCtrl |
C sCtrlBits |
▼C uLoRaMacHeader |
C sHdrBits |
C uMibParam |
C uPhyParam |
▼C uVerifyParams |
C sDatarateParams |