| SX126x-Arduino 2.0.1

Data Fields
sSetBandTxDoneParams Struct Reference
Region implementation

`#include <Region.h>`

## Data Fields
uint8_t | Channel
bool | Joined
TimerTime_t | LastTxDoneTime

## Detailed Description

Parameter structure for the function RegionSetBandTxDone.

## Field Documentation

## ◆ Channel

uint8_t sSetBandTxDoneParams::Channel

Channel to update.

## ◆ Joined

bool sSetBandTxDoneParams::Joined

Joined Set to true, if the node has joined the network

## ◆ LastTxDoneTime

TimerTime_t sSetBandTxDoneParams::LastTxDoneTime

Last TX done time.

The documentation for this struct was generated from the following file:

- src/mac/region/Region.h