| SX126x-Arduino 2.0.1

Data Fields
sDlChannelReqParams Struct Reference
Region implementation

`#include <Region.h>`

## Data Fields
uint8_t | ChannelId
uint32_t | Rx1Frequency

## Detailed Description

Parameter structure for the function RegionDlChannelReq.

## Field Documentation

## ◆ ChannelId

uint8_t sDlChannelReqParams::ChannelId

Channel Id to add the frequency.

## ◆ Rx1Frequency

uint32_t sDlChannelReqParams::Rx1Frequency

Alternative frequency for the Rx1 window.

The documentation for this struct was generated from the following file:

- src/mac/region/Region.h