| SX126x-Arduino 2.0.1

Data Fields
sLoRaMacTxInfo Struct Reference
LoRa MAC layer implementation

`#include <LoRaMac.h>`

## Data Fields
uint8_t | MaxPossiblePayload
uint8_t | CurrentPayloadSize

## Detailed Description

LoRaMAC tx information

## Field Documentation

## ◆ MaxPossiblePayload

uint8_t sLoRaMacTxInfo::MaxPossiblePayload

Defines the size of the applicative payload which can be processed

## ◆ CurrentPayloadSize

uint8_t sLoRaMacTxInfo::CurrentPayloadSize

The current payload size, dependent on the current datarate

The documentation for this struct was generated from the following file:

- src/mac/LoRaMac.h