| SX126x-Arduino 2.0.1

Data Fields
sCalcBackOffParams Struct Reference
Region implementation

`#include <Region.h>`

## Data Fields
bool | Joined
bool | LastTxIsJoinRequest
bool | DutyCycleEnabled
uint8_t | Channel
TimerTime_t | ElapsedTime
TimerTime_t | TxTimeOnAir

## Detailed Description

Parameter structure for the function RegionCalcBackOff.

## Field Documentation

## ◆ Joined

bool sCalcBackOffParams::Joined

Set to true, if the node has already joined a network, otherwise false.

## ◆ LastTxIsJoinRequest

bool sCalcBackOffParams::LastTxIsJoinRequest

Joined Set to true, if the last uplink was a join request

## ◆ DutyCycleEnabled

bool sCalcBackOffParams::DutyCycleEnabled

Set to true, if the duty cycle is enabled, otherwise false.

## ◆ Channel

uint8_t sCalcBackOffParams::Channel

Current channel index.

## ◆ ElapsedTime

TimerTime_t sCalcBackOffParams::ElapsedTime

Elapsed time since the start of the node.

## ◆ TxTimeOnAir

TimerTime_t sCalcBackOffParams::TxTimeOnAir

Time-on-air of the last transmission.

The documentation for this struct was generated from the following file:

- src/mac/region/Region.h