| SX126x-Arduino 2.0.1

region Directory Reference

## Files
file | Region.cpp
file | Region.h [code]
| Region implementation.
file | RegionAS923.cpp
file | RegionAS923.h [code]
| Region definition for AS923.
file | RegionAU915.cpp
file | RegionAU915.h [code]
| Region definition for AU915.
file | RegionCN470.cpp
file | RegionCN470.h [code]
| Region definition for CN470.
file | RegionCN779.cpp
file | RegionCN779.h [code]
| Region definition for CN779.
file | RegionCommon.cpp
file | RegionCommon.h [code]
| Region independent implementations which are common to all regions.
file | RegionEU433.cpp
file | RegionEU433.h [code]
| Region definition for EU433.
file | RegionEU868.cpp
file | RegionEU868.h [code]
| Region definition for EU868.
file | RegionIN865.cpp
file | RegionIN865.h [code]
| Region definition for IN865.
file | RegionKR920.cpp
file | RegionKR920.h [code]
| Region definition for KR920.
file | RegionRU864.cpp
file | RegionRU864.h [code]
| Region definition for RU864.
file | RegionUS915.cpp
file | RegionUS915.h [code]
| Region definition for US915.