| SX126x-Arduino 2.0.1

Data Fields
sMcpsReqProprietary Struct Reference
LoRa MAC layer implementation

`#include <LoRaMac.h>`

## Data Fields
void * | fBuffer
uint16_t | fBufferSize
int8_t | Datarate

## Detailed Description

LoRaMAC MCPS-Request for a proprietary frame

## Field Documentation

## ◆ fBuffer

void* sMcpsReqProprietary::fBuffer

Pointer to the buffer of the frame payload

## ◆ fBufferSize

uint16_t sMcpsReqProprietary::fBufferSize

Size of the frame payload

## ◆ Datarate

int8_t sMcpsReqProprietary::Datarate

Uplink datarate, if ADR is off

The documentation for this struct was generated from the following file:

- src/mac/LoRaMac.h