| SX126x-Arduino 2.0.1

Data Fields
TimerEvent_s Struct Reference

Timer object description. More...

`#include <timer.h>`

## Data Fields
uint8_t | timerNum
bool | oneShot = true
uint32_t | Timestamp
uint32_t | ReloadValue = 10000
bool | IsRunning
void(* | Callback )(void)
struct TimerEvent_s * | Next

## Detailed Description

Timer object description.

Examples
  LoRaWanPio\src\main.cpp.

## Field Documentation

## ◆ timerNum

uint8_t TimerEvent_s::timerNum

Used with ESP32 MCU 1 for TX, 2 for RX

Examples
  LoRaWanPio\src\main.cpp.

## ◆ oneShot

bool TimerEvent_s::oneShot = true

True if it is a one shot timer

## ◆ Timestamp

uint32_t TimerEvent_s::Timestamp

Current timer value

## ◆ ReloadValue

uint32_t TimerEvent_s::ReloadValue = 10000

Timer delay value

## ◆ IsRunning

bool TimerEvent_s::IsRunning

Is the timer currently running

## ◆ Callback

void(* TimerEvent_s::Callback) (void)

Timer IRQ callback function

## ◆ Next

struct TimerEvent_s* TimerEvent_s::Next

Pointer to the next Timer object.

The documentation for this struct was generated from the following file:

- src/boards/mcu/timer.h