| SX126x-Arduino 2.0.1

Data Fields
sRxConfigParams Struct Reference
Region implementation

`#include <Region.h>`

## Data Fields
uint8_t | Channel
int8_t | Datarate
uint8_t | Bandwidth
int8_t | DrOffset
uint32_t | Frequency
uint32_t | WindowTimeout
int32_t | WindowOffset
uint8_t | DownlinkDwellTime
bool | RepeaterSupport
bool | RxContinuous
bool | Window

## Detailed Description

Parameter structure for the function RegionRxConfig.

## Field Documentation

## ◆ Channel

uint8_t sRxConfigParams::Channel

The RX channel.

## ◆ Datarate

int8_t sRxConfigParams::Datarate

RX datarate.

## ◆ Bandwidth

uint8_t sRxConfigParams::Bandwidth

RX bandwidth.

## ◆ DrOffset

int8_t sRxConfigParams::DrOffset

RX datarate offset.

## ◆ Frequency

uint32_t sRxConfigParams::Frequency

RX frequency.

## ◆ WindowTimeout

uint32_t sRxConfigParams::WindowTimeout

RX window timeout

## ◆ WindowOffset

int32_t sRxConfigParams::WindowOffset

RX window offset

## ◆ DownlinkDwellTime

uint8_t sRxConfigParams::DownlinkDwellTime

Downlink dwell time.

## ◆ RepeaterSupport

bool sRxConfigParams::RepeaterSupport

Set to true, if a repeater is supported.

## ◆ RxContinuous

bool sRxConfigParams::RxContinuous

Set to true, if RX should be continuous.

## ◆ Window

bool sRxConfigParams::Window

Sets the RX window. 0: RX window 1, 1: RX window 2.

The documentation for this struct was generated from the following file:

- src/mac/region/Region.h