| SX126x-Arduino 2.0.1

Data Fields
SleepParams_t Union Reference

Represents a sleep mode configuration. More...

`#include <sx126x.h>`

## Data Fields
struct {
uint8_t WakeUpRTC: 1
| Get out of sleep mode if wakeup signal received from RTC. More...
uint8_t Reset: 1
uint8_t WarmStart: 1
uint8_t Reserved: 5
} | Fields
uint8_t | Value

## Detailed Description

Represents a sleep mode configuration.

## Field Documentation

## ◆ WakeUpRTC

uint8_t SleepParams_t::WakeUpRTC

Get out of sleep mode if wakeup signal received from RTC.

## ◆ Reset

uint8_t SleepParams_t::Reset

## ◆ WarmStart

uint8_t SleepParams_t::WarmStart

## ◆ Reserved

uint8_t SleepParams_t::Reserved

## ◆ Fields

struct { ... } SleepParams_t::Fields

## ◆ Value

uint8_t SleepParams_t::Value

The documentation for this union was generated from the following file:

- src/radio/sx126x/sx126x.h