| SX126x-Arduino 2.0.1

Data Fields
sMcpsConfirm Struct Reference
LoRa MAC layer implementation

`#include <LoRaMac.h>`

## Data Fields
Mcps_t | McpsRequest
LoRaMacEventInfoStatus_t | Status
uint8_t | Datarate
int8_t | TxPower
bool | AckReceived
uint8_t | NbRetries
TimerTime_t | TxTimeOnAir
uint32_t | UpLinkCounter
uint32_t | UpLinkFrequency

## Detailed Description

LoRaMAC MCPS-Confirm

## Field Documentation

## ◆ McpsRequest

Mcps_t sMcpsConfirm::McpsRequest

Holds the previously performed MCPS-Request

## ◆ Status

LoRaMacEventInfoStatus_t sMcpsConfirm::Status

Status of the operation

## ◆ Datarate

uint8_t sMcpsConfirm::Datarate

Uplink datarate

## ◆ TxPower

int8_t sMcpsConfirm::TxPower

Transmission power

## ◆ AckReceived

bool sMcpsConfirm::AckReceived

Set if an acknowledgement was received

## ◆ NbRetries

uint8_t sMcpsConfirm::NbRetries

Provides the number of retransmissions

## ◆ TxTimeOnAir

TimerTime_t sMcpsConfirm::TxTimeOnAir

The transmission time on air of the frame

## ◆ UpLinkCounter

uint32_t sMcpsConfirm::UpLinkCounter

The uplink counter value related to the frame

## ◆ UpLinkFrequency

uint32_t sMcpsConfirm::UpLinkFrequency

The uplink frequency related to the frame

The documentation for this struct was generated from the following file:

- src/mac/LoRaMac.h