| SX126x-Arduino 2.0.1

Data Fields
_AES_CMAC_CTX Struct Reference

`#include <cmac.h>`

## Data Fields
lora_aes_context | rijndael
uint8_t | X [16]
uint8_t | M_last [16]
uint32_t | M_n

## Field Documentation

## ◆ rijndael

lora_aes_context _AES_CMAC_CTX::rijndael

## ◆ X

uint8_t _AES_CMAC_CTX::X[16]

## ◆ M_last

uint8_t _AES_CMAC_CTX::M_last[16]

## ◆ M_n

uint32_t _AES_CMAC_CTX::M_n

The documentation for this struct was generated from the following file:

- src/system/crypto/cmac.h