| SX126x-Arduino 2.0.1

Data Fields
sContinuousWaveParams Struct Reference
Region implementation

`#include <Region.h>`

## Data Fields
uint8_t | Channel
int8_t | Datarate
int8_t | TxPower
float | MaxEirp
float | AntennaGain
uint16_t | Timeout

## Detailed Description

Parameter structure for the function RegionContinuousWave.

## Field Documentation

## ◆ Channel

uint8_t sContinuousWaveParams::Channel

Current channel index.

## ◆ Datarate

int8_t sContinuousWaveParams::Datarate

Datarate. Used to limit the TX power.

## ◆ TxPower

int8_t sContinuousWaveParams::TxPower

The TX power to setup.

## ◆ MaxEirp

float sContinuousWaveParams::MaxEirp

Max EIRP, if applicable.

## ◆ AntennaGain

float sContinuousWaveParams::AntennaGain

The antenna gain, if applicable.

## ◆ Timeout

uint16_t sContinuousWaveParams::Timeout

Specifies the time the radio will stay in CW mode.

The documentation for this struct was generated from the following file:

- src/mac/region/Region.h