| SX126x-Arduino 2.0.1

Data Fields
sMlmeReqJoin Struct Reference
LoRa MAC layer implementation

`#include <LoRaMac.h>`

## Data Fields
uint8_t * | DevEui
uint8_t * | AppEui
uint8_t * | AppKey
uint8_t | NbTrials

## Detailed Description

LoRaMAC MLME-Request for the join service

## Field Documentation

## ◆ DevEui

uint8_t* sMlmeReqJoin::DevEui

Globally unique end-device identifier

LoRaWAN Specification V1.0.2, chapter 6.2.1

## ◆ AppEui

uint8_t* sMlmeReqJoin::AppEui

Application identifier

LoRaWAN Specification V1.0.2, chapter 6.1.2

## ◆ AppKey

uint8_t* sMlmeReqJoin::AppKey

AES-128 application key

LoRaWAN Specification V1.0.2, chapter 6.2.2

## ◆ NbTrials

uint8_t sMlmeReqJoin::NbTrials

Number of trials for the join request.

The documentation for this struct was generated from the following file:

- src/mac/LoRaMac.h