| SX126x-Arduino 2.0.1

Data Fields
sLoRaMacCallback Struct Reference
LoRa MAC layer implementation

`#include <LoRaMac.h>`

## Data Fields
uint8_t(* | GetBatteryLevel )(void)
| Measures the battery level. More...

## Detailed Description

LoRaMAC callback structure

## Field Documentation

## ◆ GetBatteryLevel

uint8_t(* sLoRaMacCallback::GetBatteryLevel) (void)

Measures the battery level.

Return values

  Battery | level [0: node is connected to an external power source, 1..254: battery level, where 1 is the minimum and 254 is the maximum value, 255: the node was not able to measure the battery level]

The documentation for this struct was generated from the following file:

- src/mac/LoRaMac.h