| SX126x-Arduino 2.0.1

Data Fields
sRxParamSetupReqParams Struct Reference
Region implementation

`#include <Region.h>`

## Data Fields
int8_t | Datarate
int8_t | DrOffset
uint32_t | Frequency

## Detailed Description

Parameter structure for the function RegionRxParamSetupReq.

## Field Documentation

## ◆ Datarate

int8_t sRxParamSetupReqParams::Datarate

The datarate to setup.

## ◆ DrOffset

int8_t sRxParamSetupReqParams::DrOffset

Datarate offset.

## ◆ Frequency

uint32_t sRxParamSetupReqParams::Frequency

The frequency to setup.

The documentation for this struct was generated from the following file:

- src/mac/region/Region.h