| SX126x-Arduino 2.0.1

Data Fields
sChanMaskSetParams Struct Reference
Region implementation

`#include <Region.h>`

## Data Fields
uint16_t * | ChannelsMaskIn
ChannelsMask_t | ChannelsMaskType

## Detailed Description

Parameter structure for the function RegionChanMaskSet.

## Field Documentation

## ◆ ChannelsMaskIn

uint16_t* sChanMaskSetParams::ChannelsMaskIn

Pointer to the channels mask which should be set.

## ◆ ChannelsMaskType

ChannelsMask_t sChanMaskSetParams::ChannelsMaskType

Pointer to the channels mask which should be set.

The documentation for this struct was generated from the following file:

- src/mac/region/Region.h