| SX126x-Arduino 2.0.1

Data Fields
CalibrationParams_t Union Reference

Represents a calibration configuration. More...

`#include <sx126x.h>`

## Data Fields
struct {
uint8_t RC64KEnable: 1
| Calibrate RC64K clock. More...
uint8_t RC13MEnable: 1
| Calibrate RC13M clock. More...
uint8_t PLLEnable: 1
| Calibrate PLL. More...
uint8_t ADCPulseEnable: 1
| Calibrate ADC Pulse. More...
uint8_t ADCBulkNEnable: 1
| Calibrate ADC bulkN. More...
uint8_t ADCBulkPEnable: 1
| Calibrate ADC bulkP. More...
uint8_t ImgEnable: 1
uint8_t __pad0__: 1
} | Fields
uint8_t | Value

## Detailed Description

Represents a calibration configuration.

## Field Documentation

## ◆ RC64KEnable

uint8_t CalibrationParams_t::RC64KEnable

Calibrate RC64K clock.

## ◆ RC13MEnable

uint8_t CalibrationParams_t::RC13MEnable

Calibrate RC13M clock.

## ◆ PLLEnable

uint8_t CalibrationParams_t::PLLEnable

Calibrate PLL.

## ◆ ADCPulseEnable

uint8_t CalibrationParams_t::ADCPulseEnable

Calibrate ADC Pulse.

## ◆ ADCBulkNEnable

uint8_t CalibrationParams_t::ADCBulkNEnable

Calibrate ADC bulkN.

## ◆ ADCBulkPEnable

uint8_t CalibrationParams_t::ADCBulkPEnable

Calibrate ADC bulkP.

## ◆ ImgEnable

uint8_t CalibrationParams_t::ImgEnable

## ◆ __pad0__

uint8_t CalibrationParams_t::__pad0__

## ◆ Fields

struct { ... } CalibrationParams_t::Fields

## ◆ Value

uint8_t CalibrationParams_t::Value

The documentation for this union was generated from the following file:

- src/radio/sx126x/sx126x.h