| SX126x-Arduino 2.0.1

Data Fields
sMcpsReqUnconfirmed Struct Reference
LoRa MAC layer implementation

`#include <LoRaMac.h>`

## Data Fields
uint8_t | fPort
void * | fBuffer
uint16_t | fBufferSize
int8_t | Datarate

## Detailed Description

LoRaMAC MCPS-Request for an unconfirmed frame

## Field Documentation

## ◆ fPort

uint8_t sMcpsReqUnconfirmed::fPort

Frame port field. Must be set if the payload is not empty. Use the application specific frame port values: [1...223]

LoRaWAN Specification V1.0.2, chapter 4.3.2

## ◆ fBuffer

void* sMcpsReqUnconfirmed::fBuffer

Pointer to the buffer of the frame payload

## ◆ fBufferSize

uint16_t sMcpsReqUnconfirmed::fBufferSize

Size of the frame payload

## ◆ Datarate

int8_t sMcpsReqUnconfirmed::Datarate

Uplink datarate, if ADR is off

The documentation for this struct was generated from the following file:

- src/mac/LoRaMac.h