| SX126x-Arduino 2.0.1

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - c -

- CadDone : RadioEvents_t
- cadDone : SX126xCallbacks_t
- Callback : TimerEvent_s
- Channel : sCalcBackOffParams , sContinuousWaveParams , sRegionCommonCalcBackOffParams , sRxConfigParams , sSetBandTxDoneParams , sTxConfigParams
- ChannelId : sChannelAddParams , sChannelRemoveParams , sDlChannelReqParams , sNewChannelReqParams
- ChannelList : uMibParam
- ChannelNbRep : uMibParam
- Channels : sRegionCommonCalcBackOffParams , sRegionCommonLinkAdrReqVerifyParams , uPhyParam
- ChannelsDatarate : sLoRaMacParams , uMibParam
- ChannelsDefaultDatarate : uMibParam
- ChannelsDefaultMask : uMibParam
- ChannelsDefaultTxPower : uMibParam
- ChannelsMask : sRegionCommonLinkAdrReqVerifyParams , uMibParam , uPhyParam
- ChannelsMaskIn : sChanMaskSetParams
- ChannelsMaskType : sChanMaskSetParams
- ChannelsNbRep : sLoRaMacParams
- ChannelsTxPower : sLoRaMacParams , uMibParam
- CheckRfFrequency : Radio_s
- CHIP_TYPE : hw_config
- ChipMode : RadioStatus_u
- ChMask : sRegionCommonLinkAdrParams
- ChMaskCtrl : sRegionCommonLinkAdrParams
- Class : uMibParam
- CmdStatus : RadioStatus_u
- CodingRate : ModulationParams_t
- Confirmed : sMcpsReq::uMcpsParam
- CpuBusy : RadioStatus_u
- CrcLength : PacketParams_t
- CrcMode : PacketParams_t
- CrcOk : RxCounter_t
- Current : RadioPublicNetwork_t
- CurrentDatarate : sLinkAdrReqParams , sRegionCommonLinkAdrReqVerifyParams
- CurrentNbRep : sLinkAdrReqParams , sRegionCommonLinkAdrReqVerifyParams
- CurrentPayloadSize : sLoRaMacTxInfo
- CurrentTxPower : sLinkAdrReqParams , sRegionCommonLinkAdrReqVerifyParams