| SX126x-Arduino 2.0.1

Data Fields
RxCounter_t Struct Reference

Represents the Rx internal counters values when GFSK or LoRa packet type is used. More...

`#include <sx126x.h>`

## Data Fields
RadioPacketTypes_t | packetType
| Packet to which the packet status are referring to. More...
uint16_t | PacketReceived
uint16_t | CrcOk
uint16_t | LengthError

## Detailed Description

Represents the Rx internal counters values when GFSK or LoRa packet type is used.

## Field Documentation

## ◆ packetType

RadioPacketTypes_t RxCounter_t::packetType

Packet to which the packet status are referring to.

## ◆ PacketReceived

uint16_t RxCounter_t::PacketReceived

## ◆ CrcOk

uint16_t RxCounter_t::CrcOk

## ◆ LengthError

uint16_t RxCounter_t::LengthError

The documentation for this struct was generated from the following file:

- src/radio/sx126x/sx126x.h