| SX126x-Arduino 2.0.1

Data Fields
uPhyParam Union Reference
Region implementation

`#include <Region.h>`

## Data Fields
uint32_t | Value
float | fValue
uint16_t * | ChannelsMask
ChannelParams_t * | Channels

## Detailed Description

Union for the structure uGetPhyParams

## Field Documentation

## ◆ Value

uint32_t uPhyParam::Value

A parameter value.

## ◆ fValue

float uPhyParam::fValue

A floating point value.

## ◆ ChannelsMask

uint16_t* uPhyParam::ChannelsMask

Pointer to the channels mask.

## ◆ Channels

ChannelParams_t* uPhyParam::Channels

Pointer to the channels.

The documentation for this union was generated from the following file:

- src/mac/region/Region.h