| SX126x-Arduino 2.0.1

Data Fields
sNextChanParams Struct Reference
Region implementation

`#include <Region.h>`

## Data Fields
TimerTime_t | AggrTimeOff
TimerTime_t | LastAggrTx
int8_t | Datarate
bool | Joined
bool | DutyCycleEnabled

## Detailed Description

Parameter structure for the function RegionNextChannel.

## Field Documentation

## ◆ AggrTimeOff

TimerTime_t sNextChanParams::AggrTimeOff

Aggregated time-off time.

## ◆ LastAggrTx

TimerTime_t sNextChanParams::LastAggrTx

Time of the last aggregated TX.

## ◆ Datarate

int8_t sNextChanParams::Datarate

Current datarate.

## ◆ Joined

bool sNextChanParams::Joined

Set to true, if the node has already joined a network, otherwise false.

## ◆ DutyCycleEnabled

bool sNextChanParams::DutyCycleEnabled

Set to true, if the duty cycle is enabled, otherwise false.

The documentation for this struct was generated from the following file:

- src/mac/region/Region.h