| SX126x-Arduino 2.0.1

Data Fields
lmh_param_s Struct Reference

`#include <LoRaMacHelper.h>`

## Data Fields
bool | adr_enable
int8_t | tx_data_rate
bool | enable_public_network
uint8_t | nb_trials
int8_t | tx_power
bool | duty_cycle

## Detailed Description

Examples
  LoRaWanPio\src\main.cpp.

## Field Documentation

## ◆ adr_enable

bool lmh_param_s::adr_enable

Activation state of adaptative Datarate

## ◆ tx_data_rate

int8_t lmh_param_s::tx_data_rate

Uplink datarate, if AdrEnable is off

## ◆ enable_public_network

bool lmh_param_s::enable_public_network

Enable or disable a public network

## ◆ nb_trials

uint8_t lmh_param_s::nb_trials

Number of trials for the join request.

## ◆ tx_power

int8_t lmh_param_s::tx_power

Uplink power

## ◆ duty_cycle

bool lmh_param_s::duty_cycle

Enable or disable the duty cycle control

The documentation for this struct was generated from the following file:

- src/mac/LoRaMacHelper.h