| SX126x-Arduino 2.0.1

Todo List

Global SX126xWaitOnBusy (void)
  This error should be reported to the main app
Global OnRadioRxDone (uint8_t *payload, uint16_t size, int16_t rssi, int8_t snr)
  need callback for confirmed down
Global LoRaMacInitialization (LoRaMacPrimitives_t *primitives, LoRaMacCallback_t *callbacks, LoRaMacRegion_t region, eDeviceClass nodeClass=CLASS_A)
  Putting the RegionTxConfig here makes the OTAA join more stable
Global AS923_NUMB_CHANNELS_CF_LIST
  should be 6
Global RU864_NUMB_CHANNELS_CF_LIST
  should be 6