AceTime 2.4.0 Date and time classes for Arduino that support timezones from the TZ Database.

List of all members
ace_time::ExtendedZoneProcessorCache< SIZE > Class Template Reference

An implementation of an ExtendedZoneProcessorCacheBase where the cache of size SIZE is embedded into the class itself. More...

`#include <ZoneProcessorCache.h>`

Inheritance diagram for ace_time::ExtendedZoneProcessorCache< SIZE >:
[legend]
Collaboration diagram for ace_time::ExtendedZoneProcessorCache< SIZE >:
[legend]

## Additional Inherited Members
Public Member Functions inherited from ace_time::ZoneProcessorCacheBaseTemplate< ZP >
| ZoneProcessorCacheBaseTemplate (ZP *zoneProcessors, uint8_t size)
uint8_t | size () const
| Return the size of the cache.
ZP * | getZoneProcessorAtIndex (uint8_t i)
| Get the ZoneProcessor at index i.
ZP * | getZoneProcessor (uintptr_t zoneKey)
| Get ZoneProcessor from either a ZoneKey, either a basic::ZoneInfo or an extended::ZoneInfo. More...

## Detailed Description

### template<uint8_t SIZE>
class ace_time::ExtendedZoneProcessorCache< SIZE >

An implementation of an ExtendedZoneProcessorCacheBase where the cache of size SIZE is embedded into the class itself.

This is expected to be created as a global object and passed into the ExtendedZoneManager.

Template Parameters

  SIZE | number of zone processors, should be approximate the number zones concurrently used in the app. It is expected that this will be small. It can be 1 if the app never changes the TimeZone. It should be 2 if the user is able to select different timezones from a menu.

Definition at line 147 of file ZoneProcessorCache.h.

The documentation for this class was generated from the following file:

- /home/brian/src/AceTime/src/ace_time/ZoneProcessorCache.h