AceTime 2.4.0 Date and time classes for Arduino that support timezones from the TZ Database.

Public Member Functions | List of all members
ace_time::ManualZoneManager Class Reference

A simple version of ZoneManager that converts a manual TimeZoneData with fixed STD and DST offsets into a TimeZone. More...

`#include <ZoneManager.h>`

## Public Member Functions
TimeZone | createForTimeZoneData (const TimeZoneData &d)
| Create a TimeZone with fixed STD and DST offsets stored in the TimeZoneData which was created by TimeZone::toTimeZoneData(). More...
uint16_t | zoneRegistrySize () const

## Detailed Description

A simple version of ZoneManager that converts a manual TimeZoneData with fixed STD and DST offsets into a TimeZone.

Definition at line 40 of file ZoneManager.h.

## Member Function Documentation

## ◆ createForTimeZoneData()

TimeZone ace_time::ManualZoneManager::createForTimeZoneData | ( | const TimeZoneData & | d | ) |
| inline

Create a TimeZone with fixed STD and DST offsets stored in the TimeZoneData which was created by TimeZone::toTimeZoneData().

IANA timezones are not supported.

Definition at line 47 of file ZoneManager.h.

The documentation for this class was generated from the following file:

- /home/brian/src/AceTime/src/ace_time/ZoneManager.h