# Memory Benchmark

The `MemoryBenchmark.ino` was compiled with each `FEATURE_*` and the flash
memory and static RAM sizes were recorded. The `FEATURE_BASELINE` selection is
the baseline, and its memory usage  numbers are subtracted from the subsequent
`FEATURE_*` memory usage.

**Version**: AceTime v2.4.0

**DO NOT EDIT**: This file was auto-generated using `make README.md`.

## How to Regenerate

To regenerate this README.md:

```
$ make clean_benchmarks
$ make benchmarks
$ make README.md
```

The `make benchmarks` target uses `collect.sh` script which calls `auniter.sh`
(https://github.com/bxparks/AUniter) to invoke the Arduino IDE programmatically.
It produces a `*.txt` file with the flash and ram usage information (e.g.
`nano.txt`). It now takes about 16 minutes to generate the `*.txt` files on my
quad-core Intel Core i7-3840QM CPU @ 2.80GHz laptop.

The `make README.md` command calls the `generated_readme.py` Python script which
generates this `README.md` file. The ASCII tables below are generated by the
`generate_table.awk` script, which takes each `*.txt` file and converts it to an
ASCII table.

## Library Size Changes

**v1.3:**
* The `BasicZoneManager` and `ExtendedZoneManager` classes were unified under a
  new parent interface `ZoneManager`. This seems to have caused the flash size
  to increase by around 1200 bytes on the AVR processors (Nano, Pro Micro),
  about 500 bytes on a SAMD, about 800 bytes on a ESP8266, 100 bytes on a ESP32,
  and 1400 bytes on a Teensy 3.2. The 8-bit processors suffer the most flash
  size increase proportional to their limited 32kB limit.
* Adding the `ZoneManager` interface simplifies a lot of the complexity with
  saving and restoring time zones using the `TimeZoneData` object, and I think
  it is worth the extra cost of flash size. The mitigating factor is that
  applications targetted towards 8-bit processors will normally have fixed
  number of timezones at compile time, so they can avoid using a `ZoneManager`,
  and avoid this penalty in flash size.

**v1.4.1+:**
* Removed the `ZoneInfo::transitionBufSize` field from the `ZoneInfo` struct,
  which saves 1 byte on 8-bit processors (none on 32-bit processors due to
  4-byte alignment). We save 266 bytes for `BasicZoneManager` and 386 bytes for
  `ExtendedZoneManager` when all the zones are loaded into the zone registry.
* Incorporated zoneName compression causes flash/ram usage to increase by
  ~250/120 bytes when using only 1-2 zones, but *decreases* flash consumption by
  1200-2400 bytes when all the zones are loaded into the `ZoneManager`.

**v1.5+:**
* Changing `ZoneProcessorCache::getType()` from a `virtual` to a non-virtual
  method saves 250-350 bytes of flash memory when using a `BasicZoneManager` or
  an `ExtendedZoneManager` on an 8-bit AVR processor. Unexpectedly, the flash
  memory consumption *increases* slightly (~0-50 bytes) for some ARM processors
  and the ESP32. Since those processors have far more flash memory, this seems
  like a good tradeoff.
* Changing `BasicZoneProcessor` and `ExtendedZoneProcessor` to be subclasses of
  the templatized `BasicZoneProcessorTemplate` and
  `ExtendedZoneProcessorTemplate` classes causes reduction of flash consumption
  by 250-400 bytes for 32-bit processors. Don't know why. (Very little
  difference for 8-bit AVR).
* Adding a `ZoneInfoStore` layer of indirection (to support more complex
  ZoneProcessors and Brokers) causes flash memory to go up by 100-200 bytes.

**v1.6:**
* Added support for `LinkRegistry` to `BasicZoneManager` and
  `ExtendedZoneManager`. This increases the flash memory usage by 150-500 bytes
  when using one of these classes due to the code required by `LinkRegistrar`. This extra cost is incurred even if the `LinkRegistry` is set to 0 elements. Each `LinkEntry` consumes 8 bytes (2 x `uint32_t`). So a
  `zonedb::kLinkRegistry` with 183 elements uses 1464 extra bytes of flash; a
  `zonedbx::kLinkRegistry` with 207 elements uses 1656 extra bytes.

**v1.7:**
* The virtual destructor on the `Clock` base class removed. This reduced the
  flash usage by 618 bytes on AVR processors , 328 bytes on the SAMD21, but only
  50-60 bytes on other 32-bit processors.
* The various `printShortNameTo()` or `printShortTo()` methods changed to
  replace the underscore in the zone names (e.g. `Los_Angeles`) with spaces
  (e.g. `Los Angeles`) to be more human friendly. This made little difference in
  the flash memory consumption, except on the ESP32 where it increased by
  200-300 bytes.

**v1.7.2**
* The `SystemClock::clockMillis()` is now non-virtual, using compile-time
  polymorphism through C++ template, and incorporating the same techniques from
  AceRoutine v1.3. Saves about 20-40 bytes of flash.

**v1.7.5:**
* `ExtendedZoneProcessor.compareTransitionToMatch()` was modified to
  detect an exact equality between a `Transition` and its `MatchingEra` if any
  of the 3 time stamp versions ('w', 's', 'u') are equal. Adds about 120-150
  bytes of flash on 8-bit and 32-bit processors. But removing
  `originalTransitionTime` from `Transition` decreases flash usage by about 20
  bytes.
* Upgrade ESP8266 Boards from 2.7.4 to 3.0.2. Flash consumption increases by
  3-5 kB across the board.
* Upgrade Teensyduino from 1.54 to 1.55. Add memory consumed by `malloc()` and
  `free()` when using classes with virtual methods into baseline
  MemoryBenchmark, reducing the actual memory usage of various features by
  ~3kB.

**v1.8.0:**
* Move Clock and SystemClock benchmarks into AceTimeClock v1.0.0.
* Extract thin links from BasicZoneManager and ExtendedZoneManager into
  new BasicLinkManager and ExtendedLinkManager classes.
    * Saves 200-500 bytes of flash for BasicZoneManager and ExtendedZoneManager.
    * Applications can decide whether to use thin links through the LinkManager
      (~2000 flash bytes for AVR) or use fat links through the
      `kZoneAndLinkRegistry` (~5000 flash bytes for AVR).
* Create various test objects as global variables instead of stack variables
  to get a more accurate measurement of their static memory consumption.

**v1.9.0:**
* Reduce flash usage of `BasicZoneManager` and `ExtendedZoneManager` by
  1100-1300 bytes on AVR processors:
    * Extract `BasicZoneProcessorCache` and `ExtendedZoneProcessorCache` out
      of `BasicZoneManager` and `ExtendedZoneManager`, making them
      non-templatized.
    * Remove all `virtual` methods from `ZoneManager`, making the ZoneManager
      hierarchy non-polymorphic.
    * Looks like I am reverting some of the changes made in v1.3 when I created
      the `ZoneManager` interface.
* Reduce flash usage of `BasicLinkManager` and `ExtendedLinkManager` by
  68 bytes on AVR processors by removing pure `virtual` methods on `LinkManager`
  base class.
* Increase flash usage by 34 bytes on AVR processors due to slight refactoring
  of `getHighWater()` with `getAllocSize()`. Only 4-8 bytes increase on 32-bit
  processors.

**v1.10.0:**
* Remove support for SAMD21 boards.
    * Arduino IDE 1.8.19 with SparkFun SAMD 1.8.6 can no longer upload binaries
      to these boards. Something about bossac 1.7.0 not found.
* Add memory consumption benchmarks for `ZoneSorterByName` and
  `ZoneSorterByOffsetAndName` for `BasicZoneManager` and `ExtendedZoneManager`.
    * AVR: 180-530 bytes of flash
    * 32-bit: 120-600 bytes of flash
* Upgrade tool chain:
    * Arduino IDE from 1.8.13 to 1.8.19
    * Arduino AVR from 1.8.3 to 1.8.4
    * STM32duino from 2.0.0 to 2.2.0
    * ESP32 from 1.0.6 to 2.0.2
    * Teensyduino from 1.55 to 1.56
* Add support for `fold` parameter in `LocalDateTime`, `OffsetDateTime`,
  `ZonedDateTime`, and `ExtendedZoneProcessor`. Increases flash usage:
    * AVR:
        * ~600 bytes, in `ExtendedZoneProcessor` for additional search logic,
        * ~150 bytes, `BasicZoneProcessor`, to carry along the `fold` parameter
    * most 32-bit: 400-600 bytes
    * Teensy: 1300 bytes (no idea why)

**v1.11.0**
* Upgrade ZoneInfo database so that Links are symbolic links to Zones, instead
  of hard links to Zones.
    * Allows Links to know whether they are links.
    * Allows extraction of the zoneId and zoneNames of the target Zone.
    * AVR: Increases flash consumption by ~270 bytes.
    * STM32: Increases flash by 120-150 bytes.
    * ESP8266: Increases flash by 250-300 bytes.
    * ESP32: Increases flash by ~190 bytes.
    * Teensy 3.2: Increase flash by 450-1300 bytes.

**v1.11.1**
* Change `ZoneInfoBroker::targetZoneInfo()` method to return a `ZoneInfoBroker`
  instead of raw `ZoneInfo*` pointer.
    * Increases flash usage by 4-16 bytes for the most part.

**v1.11.5**
* Upgrade tool chain
    * Arduino CLI from 0.20.2 to 0.27.1
    * Arduino AVR Boards from 1.8.4 to 1.8.5
    * STM32duino from 2.2.0 to 2.3.0
    * ESP32 Boards from 2.0.2 to 2.0.5
    * Teensyduino from 1.56 to 1.57
* Upgrade TZDB from 2022b to 2022d

**v2.0**
* Use `int16_t` year fields.
* Implement adjustable epoch year.
* Upgrade to TZDB 2022f.
* AVR:
    * BasicZoneManager increases ~200 bytes
    * ExtendedZoneManager increases ~500 bytes
    * `zonedb` increases ~1.5 kiB
    * `zonedbx` increases ~3 kiB
* ESP8266
    * BasicZoneManager increases ~50 bytes
    * ExtendedZoneManager increases ~150 bytes
    * `zonedb` increases ~300 bytes
    * `zonedbx` increases ~1.5 kiB

**v2.0.1**
* Upgrade to TZDB 2022g.
* Incorporate `ZonedExtra` to replace various `TimeZone` methods.

**v2.1.0**
* Remove `LinkManager` and `LinkRegistry`.
* Unify links, adding an additional `targetInfo` field in `ZoneInfo`.
    * Increases flash by ~1kB on 8-bit and ~2kB on 32-bit for ~600 zones.

**v2.1.1+**
* Simplify ZoneRule.letter handling to use ZoneRule.letterIndex for all letters,
  not just ones over 1 character long. On 8-bit AVR:
    * BasicZoneProcessor
        * Increases flash consumption for 1-2 zones by ~200 bytes.
        * No change for the full TZ database.
    * ExtendedZoneProcessor
        * No change for 1-2 zones.
        * Decreases flash consumption by ~300 bytes for full TZ database.

**v2.2.0**
* Upgrade tool chain
    * Arduino AVR from 1.8.5 to 1.8.6
    * STM32duino from 2.3.0 to 2.4.0
    * ESP8266 from 3.0.2 to 3.1.2 failed, reverted back to 3.0.2
    * ESP32 from 2.0.5 to 2.0.7
* Add support for Seeed XIAO SAMD21
    * Using Seeeduino SAMD Boards 1.8.3
* Upgrade to TZDB 2023b

**v2.2.2**
* Upgrade to TZDB 2023c

**v2.2.3**
* Add support for Adafruit ItsyBitsy M4
    * Using Adafruit SAMD Boards 1.7.11
* Remove Teensy 3.2
    * Nearing end of life. Moved to Tier 2 (should work).
* Upgrade tool chain
    * Seeeduino SAMD Boards 1.8.4
    * STM32duino Boards 2.5.0
    * ESP32 Boards 2.0.9

**v2.3.0**
* Implement 1-second resolution in ExtendedZoneProcessor (decoupled from
  zonedbx storage format).
    * Increases flash usage by ~1kB on 8-bit processors, but only 0-100 bytes
      on 32-bit processors.
    * Enables it to be also used as the CompleteZoneProcessor class.
* Implement CompleteZoneProcessor as a specialization of ExtendedZoneProcessor.
    * Enables the creation of `zonedbc` database which contains all TZDB
      timezones, for all years going back to 1844, the earliest transition in
      the TZDB.
    * The flash consumption of zonedbc is roughly 2X of zonedbx.
* Revert `zonedb` to use 8-bit year fields.
    * Increases flash memory consumption for BasicZoneManager w/ 1 zone by
      around 150 bytes.
    * Decreases flash memory cosumption for BasicZoneManager w/ all timezones by
      800-900 bytes.
* Revert `zonedbx` to use 8-bit year fields.
    * Increase flash memory consumption of ExtendedZoneManager w/ 1 zone by
      around 220 bytes.
    * Decreases flash memory cosumption for ExtendedZoneManager w/ all timezones
      by ~2000 bytes.
* Move ZoneContext and its string arrays into PROGMEM.
    * Reduces RAM usage by 150-200 bytes on AVR and ESP8266 processors.
* Merge `createAbbreviation()` of BasicZoneProcessor and ExtendedZoneProcessor
    * `BasicZoneProcessor`: Slight (30-60 bytes) increase in flash memory,
      no change in RAM usage.
    * `ExtendedZoneProcessor`: Slight (30-60 bytes) increase in flash memory.
      But saves ~16 bytes of RAM for 8-bit, ~64 bytes of RAM for 32-bit.
* Support multi-character `ZoneRule.letter` field
    * Enables `Africa/Windhoek` and `America/Belize` in the `zonedb` database
      used with `BasicZoneProcessor`.
    * Increases flash memory for `zonedb` by ~150 bytes on 8-bit, ~200 on 32-bit
      processors.

**v2.4.0**
* Support %z format.
* Upgrade to TZDB 2024b.
* Upgrade Arduino CLI to 1.1.1
* AVR:
    * BasicZoneManager increases ~600 bytes
    * ExtendedZoneManager increases ~700 bytes
    * `zonedb` *decreases* ~400 bytes
    * `zonedbx` *decreases* ~350 bytes
* ESP8266
    * BasicZoneManager increases ~500 bytes
    * ExtendedZoneManager increases ~400 bytes
    * `zonedb` *decreases* ~300 bytes
    * `zonedbx` *decreases* ~100 kiB

# Legend

* [1] Delta flash and ram consumption for `Basic ZoneSorterByName` and
  `Basic ZoneSorterByOffsetAndName` are calculated by subtracting the
  `BasicZoneManager (1 zone)` numbers, to isolate the memory consumption
  of just the sorter classes.
* [2] Delta flash and ram consumption for `Extended ZoneSorterByName` and
  `Extended ZoneSorterByOffsetAndName` are calculated by subtracting the
  `ExtendedZoneManager (1 zone)` numbers, to isolate the memory
  consumption of just the sorter classes.
* [3] Delta flash and ram consumption for `Complete ZoneSorterByName` and
  `Complete ZoneSorterByOffsetAndName` are calculated by subtracting the
  `CompleteZoneManager (1 zone)` numbers, to isolate the memory
  consumption of just the sorter classes.
* An entry of `-1` indicates that the memory usage exceeded the maximum of the
  microcontroller and the compiler did not generate the desired information.

## Arduino Nano

* 16MHz ATmega328P
* Arduino IDE 1.8.19, Arduino CLI 1.1.1
* Arduino AVR Boards 1.8.6

```
+----------------------------------------------------------------------+
| Functionality                          |  flash/  ram |        delta |
|----------------------------------------+--------------+--------------|
| baseline                               |    474/   11 |      0/    0 |
|----------------------------------------+--------------+--------------|
| LocalDateTime                          |   1108/   21 |    634/   10 |
| ZonedDateTime                          |   1444/   30 |    970/   19 |
| Manual ZoneManager                     |   1406/   13 |    932/    2 |
|----------------------------------------+--------------+--------------|
| Basic TimeZone (1 zone)                |   8238/  225 |   7764/  214 |
| Basic TimeZone (2 zones)               |   8784/  379 |   8310/  368 |
| BasicZoneManager (1 zone)              |   8448/  236 |   7974/  225 |
| BasicZoneManager (all zones)           |  19646/  386 |  19172/  375 |
| BasicZoneManager (all zones+links)     |  25254/  386 |  24780/  375 |
|----------------------------------------+--------------+--------------|
| Basic ZoneSorterByName [1]             |   9222/  238 |    774/    2 |
| Basic ZoneSorterByOffsetAndName [1]    |   9344/  238 |    896/    2 |
|----------------------------------------+--------------+--------------|
| Extended TimeZone (1 zone)             |  12072/  643 |  11598/  632 |
| Extended TimeZone (2 zones)            |  12670/ 1215 |  12196/ 1204 |
| ExtendedZoneManager (1 zone)           |  12252/  649 |  11778/  638 |
| ExtendedZoneManager (all zones)        |  34680/  847 |  34206/  836 |
| ExtendedZoneManager (all zones+links)  |  40940/  847 |  40466/  836 |
|----------------------------------------+--------------+--------------|
| Extended ZoneSorterByName [2]          |  13022/  651 |    770/    2 |
| Extended ZoneSorterByOffsetAndName [2] |  13116/  651 |    864/    2 |
|----------------------------------------+--------------+--------------|
| Complete TimeZone (1 zone)             |     -1/   -1 |     -1/   -1 |
| Complete TimeZone (2 zones)            |     -1/   -1 |     -1/   -1 |
| CompleteZoneManager (1 zone)           |     -1/   -1 |     -1/   -1 |
| CompleteZoneManager (all zones)        |     -1/   -1 |     -1/   -1 |
| CompleteZoneManager (all zones+links)  |     -1/   -1 |     -1/   -1 |
|----------------------------------------+--------------+--------------|
| Complete ZoneSorterByName [3]          |     -1/   -1 |      0/    0 |
| Complete ZoneSorterByOffsetAndName [3] |     -1/   -1 |      0/    0 |
+---------------------------------------------------------------------+

```

## Sparkfun Pro Micro

* 16 MHz ATmega32U4
* Arduino IDE 1.8.19, Arduino CLI 1.1.1
* SparkFun AVR Boards 1.1.13

```
+----------------------------------------------------------------------+
| Functionality                          |  flash/  ram |        delta |
|----------------------------------------+--------------+--------------|
| baseline                               |   3470/  153 |      0/    0 |
|----------------------------------------+--------------+--------------|
| LocalDateTime                          |   4080/  161 |    610/    8 |
| ZonedDateTime                          |   4416/  170 |    946/   17 |
| Manual ZoneManager                     |   4400/  153 |    930/    0 |
|----------------------------------------+--------------+--------------|
| Basic TimeZone (1 zone)                |  11210/  365 |   7740/  212 |
| Basic TimeZone (2 zones)               |  11738/  517 |   8268/  364 |
| BasicZoneManager (1 zone)              |  11420/  376 |   7950/  223 |
| BasicZoneManager (all zones)           |  22618/  526 |  19148/  373 |
| BasicZoneManager (all zones+links)     |  28226/  526 |  24756/  373 |
|----------------------------------------+--------------+--------------|
| Basic ZoneSorterByName [1]             |  12194/  378 |    774/    2 |
| Basic ZoneSorterByOffsetAndName [1]    |  12316/  378 |    896/    2 |
|----------------------------------------+--------------+--------------|
| Extended TimeZone (1 zone)             |  15028/  783 |  11558/  630 |
| Extended TimeZone (2 zones)            |  15624/ 1353 |  12154/ 1200 |
| ExtendedZoneManager (1 zone)           |  15208/  789 |  11738/  636 |
| ExtendedZoneManager (all zones)        |  37652/  987 |  34182/  834 |
| ExtendedZoneManager (all zones+links)  |  43912/  987 |  40442/  834 |
|----------------------------------------+--------------+--------------|
| Extended ZoneSorterByName [2]          |  15978/  791 |    770/    2 |
| Extended ZoneSorterByOffsetAndName [2] |  16072/  791 |    864/    2 |
|----------------------------------------+--------------+--------------|
| Complete TimeZone (1 zone)             |     -1/   -1 |     -1/   -1 |
| Complete TimeZone (2 zones)            |     -1/   -1 |     -1/   -1 |
| CompleteZoneManager (1 zone)           |     -1/   -1 |     -1/   -1 |
| CompleteZoneManager (all zones)        |     -1/   -1 |     -1/   -1 |
| CompleteZoneManager (all zones+links)  |     -1/   -1 |     -1/   -1 |
|----------------------------------------+--------------+--------------|
| Complete ZoneSorterByName [3]          |     -1/   -1 |      0/    0 |
| Complete ZoneSorterByOffsetAndName [3] |     -1/   -1 |      0/    0 |
+---------------------------------------------------------------------+

```

## Seeed Studio XIAO SAMD21

* SAMD21, 48 MHz ARM Cortex-M0+
* Arduino IDE 1.8.19, Arduino CLI 1.1.1
* Seeeduino SAMD Boards 1.8.4

```
+----------------------------------------------------------------------+
| Functionality                          |  flash/  ram |        delta |
|----------------------------------------+--------------+--------------|
| baseline                               |  34068/    0 |      0/    0 |
|----------------------------------------+--------------+--------------|
| LocalDateTime                          |  34372/    0 |    304/    0 |
| ZonedDateTime                          |  35116/    0 |   1048/    0 |
| Manual ZoneManager                     |  35100/    0 |   1032/    0 |
|----------------------------------------+--------------+--------------|
| Basic TimeZone (1 zone)                |  39204/    0 |   5136/    0 |
| Basic TimeZone (2 zones)               |  39564/    0 |   5496/    0 |
| BasicZoneManager (1 zone)              |  39308/    0 |   5240/    0 |
| BasicZoneManager (all zones)           |  54588/    0 |  20520/    0 |
| BasicZoneManager (all zones+links)     |  63212/    0 |  29144/    0 |
|----------------------------------------+--------------+--------------|
| Basic ZoneSorterByName [1]             |  39804/    0 |    496/    0 |
| Basic ZoneSorterByOffsetAndName [1]    |  39868/    0 |    560/    0 |
|----------------------------------------+--------------+--------------|
| Extended TimeZone (1 zone)             |  41236/    0 |   7168/    0 |
| Extended TimeZone (2 zones)            |  41596/    0 |   7528/    0 |
| ExtendedZoneManager (1 zone)           |  41340/    0 |   7272/    0 |
| ExtendedZoneManager (all zones)        |  71548/    0 |  37480/    0 |
| ExtendedZoneManager (all zones+links)  |  81148/    0 |  47080/    0 |
|----------------------------------------+--------------+--------------|
| Extended ZoneSorterByName [2]          |  41828/    0 |    488/    0 |
| Extended ZoneSorterByOffsetAndName [2] |  41892/    0 |    552/    0 |
|----------------------------------------+--------------+--------------|
| Complete TimeZone (1 zone)             |  41604/    0 |   7536/    0 |
| Complete TimeZone (2 zones)            |  42828/    0 |   8760/    0 |
| CompleteZoneManager (1 zone)           |  41708/    0 |   7640/    0 |
| CompleteZoneManager (all zones)        | 120788/    0 |  86720/    0 |
| CompleteZoneManager (all zones+links)  | 130388/    0 |  96320/    0 |
|----------------------------------------+--------------+--------------|
| Complete ZoneSorterByName [3]          |  42196/    0 |    488/    0 |
| Complete ZoneSorterByOffsetAndName [3] |  42252/    0 |    544/    0 |
+---------------------------------------------------------------------+

```

## STM32 Blue Pill

* STM32F103C8, 72 MHz ARM Cortex-M3
* Arduino IDE 1.8.19, Arduino CLI 1.1.1
* STM32duino 2.5.0

```
+----------------------------------------------------------------------+
| Functionality                          |  flash/  ram |        delta |
|----------------------------------------+--------------+--------------|
| baseline                               |  21348/ 4376 |      0/    0 |
|----------------------------------------+--------------+--------------|
| LocalDateTime                          |  21704/ 4392 |    356/   16 |
| ZonedDateTime                          |  21784/ 4408 |    436/   32 |
| Manual ZoneManager                     |  22360/ 4384 |   1012/    8 |
|----------------------------------------+--------------+--------------|
| Basic TimeZone (1 zone)                |  26404/ 4592 |   5056/  216 |
| Basic TimeZone (2 zones)               |  26776/ 4800 |   5428/  424 |
| BasicZoneManager (1 zone)              |  26524/ 4612 |   5176/  236 |
| BasicZoneManager (all zones)           |  42180/ 4612 |  20832/  236 |
| BasicZoneManager (all zones+links)     |  51080/ 4612 |  29732/  236 |
|----------------------------------------+--------------+--------------|
| Basic ZoneSorterByName [1]             |  26992/ 4616 |    468/    4 |
| Basic ZoneSorterByOffsetAndName [1]    |  27076/ 4616 |    552/    4 |
|----------------------------------------+--------------+--------------|
| Extended TimeZone (1 zone)             |  28188/ 5148 |   6840/  772 |
| Extended TimeZone (2 zones)            |  28564/ 5912 |   7216/ 1536 |
| ExtendedZoneManager (1 zone)           |  28304/ 5156 |   6956/  780 |
| ExtendedZoneManager (all zones)        |  59096/ 5156 |  37748/  780 |
| ExtendedZoneManager (all zones+links)  |  69040/ 5156 |  47692/  780 |
|----------------------------------------+--------------+--------------|
| Extended ZoneSorterByName [2]          |  28768/ 5160 |    464/    4 |
| Extended ZoneSorterByOffsetAndName [2] |  28840/ 5160 |    536/    4 |
|----------------------------------------+--------------+--------------|
| Complete TimeZone (1 zone)             |  28568/ 5148 |   7220/  772 |
| Complete TimeZone (2 zones)            |  29804/ 5912 |   8456/ 1536 |
| CompleteZoneManager (1 zone)           |  28684/ 5156 |   7336/  780 |
| CompleteZoneManager (all zones)        | 108204/ 5156 |  86856/  780 |
| CompleteZoneManager (all zones+links)  | 118148/ 5156 |  96800/  780 |
|----------------------------------------+--------------+--------------|
| Complete ZoneSorterByName [3]          |  29148/ 5160 |    464/    4 |
| Complete ZoneSorterByOffsetAndName [3] |  29220/ 5160 |    536/    4 |
+---------------------------------------------------------------------+

```

## SAMD51 (Adafruit ItsyBitsy M4)

* SAMD51, 120 MHz ARM Cortex-M4
* Arduino IDE 1.8.19, Arduino CLI 1.1.1
* Adafruit SAMD 1.7.11

```
+----------------------------------------------------------------------+
| Functionality                          |  flash/  ram |        delta |
|----------------------------------------+--------------+--------------|
| baseline                               |  10580/    0 |      0/    0 |
|----------------------------------------+--------------+--------------|
| LocalDateTime                          |  10872/    0 |    292/    0 |
| ZonedDateTime                          |  11544/    0 |    964/    0 |
| Manual ZoneManager                     |  11536/    0 |    956/    0 |
|----------------------------------------+--------------+--------------|
| Basic TimeZone (1 zone)                |  15640/    0 |   5060/    0 |
| Basic TimeZone (2 zones)               |  16008/    0 |   5428/    0 |
| BasicZoneManager (1 zone)              |  15760/    0 |   5180/    0 |
| BasicZoneManager (all zones)           |  31044/    0 |  20464/    0 |
| BasicZoneManager (all zones+links)     |  39664/    0 |  29084/    0 |
|----------------------------------------+--------------+--------------|
| Basic ZoneSorterByName [1]             |  16248/    0 |    488/    0 |
| Basic ZoneSorterByOffsetAndName [1]    |  16300/    0 |    540/    0 |
|----------------------------------------+--------------+--------------|
| Extended TimeZone (1 zone)             |  17452/    0 |   6872/    0 |
| Extended TimeZone (2 zones)            |  17828/    0 |   7248/    0 |
| ExtendedZoneManager (1 zone)           |  17568/    0 |   6988/    0 |
| ExtendedZoneManager (all zones)        |  47784/    0 |  37204/    0 |
| ExtendedZoneManager (all zones+links)  |  57384/    0 |  46804/    0 |
|----------------------------------------+--------------+--------------|
| Extended ZoneSorterByName [2]          |  18056/    0 |    488/    0 |
| Extended ZoneSorterByOffsetAndName [2] |  18108/    0 |    540/    0 |
|----------------------------------------+--------------+--------------|
| Complete TimeZone (1 zone)             |  17792/    0 |   7212/    0 |
| Complete TimeZone (2 zones)            |  19028/    0 |   8448/    0 |
| CompleteZoneManager (1 zone)           |  17908/    0 |   7328/    0 |
| CompleteZoneManager (all zones)        |  96988/    0 |  86408/    0 |
| CompleteZoneManager (all zones+links)  | 106596/    0 |  96016/    0 |
|----------------------------------------+--------------+--------------|
| Complete ZoneSorterByName [3]          |  18396/    0 |    488/    0 |
| Complete ZoneSorterByOffsetAndName [3] |  18444/    0 |    536/    0 |
+---------------------------------------------------------------------+

```

## ESP8266

* NodeMCU 1.0, 80MHz ESP8266
* Arduino IDE 1.8.19, Arduino CLI 1.1.1
* ESP8266 Boards 3.0.2

```
+----------------------------------------------------------------------+
| Functionality                          |  flash/  ram |        delta |
|----------------------------------------+--------------+--------------|
| baseline                               | 260089/27892 |      0/    0 |
|----------------------------------------+--------------+--------------|
| LocalDateTime                          | 260613/27912 |    524/   20 |
| ZonedDateTime                          | 261573/27928 |   1484/   36 |
| Manual ZoneManager                     | 261553/27900 |   1464/    8 |
|----------------------------------------+--------------+--------------|
| Basic TimeZone (1 zone)                | 267625/28292 |   7536/  400 |
| Basic TimeZone (2 zones)               | 268025/28500 |   7936/  608 |
| BasicZoneManager (1 zone)              | 267785/28316 |   7696/  424 |
| BasicZoneManager (all zones)           | 283465/28316 |  23376/  424 |
| BasicZoneManager (all zones+links)     | 292361/28316 |  32272/  424 |
|----------------------------------------+--------------+--------------|
| Basic ZoneSorterByName [1]             | 268521/28316 |    736/    0 |
| Basic ZoneSorterByOffsetAndName [1]    | 268665/28316 |    880/    0 |
|----------------------------------------+--------------+--------------|
| Extended TimeZone (1 zone)             | 270073/28900 |   9984/ 1008 |
| Extended TimeZone (2 zones)            | 270489/29660 |  10400/ 1768 |
| ExtendedZoneManager (1 zone)           | 270217/28908 |  10128/ 1016 |
| ExtendedZoneManager (all zones)        | 301033/28908 |  40944/ 1016 |
| ExtendedZoneManager (all zones+links)  | 310985/28908 |  50896/ 1016 |
|----------------------------------------+--------------+--------------|
| Extended ZoneSorterByName [2]          | 270969/28908 |    752/    0 |
| Extended ZoneSorterByOffsetAndName [2] | 271017/28908 |    800/    0 |
|----------------------------------------+--------------+--------------|
| Complete TimeZone (1 zone)             | 270393/29092 |  10304/ 1200 |
| Complete TimeZone (2 zones)            | 271673/29852 |  11584/ 1960 |
| CompleteZoneManager (1 zone)           | 270537/29100 |  10448/ 1208 |
| CompleteZoneManager (all zones)        | 350089/29100 |  90000/ 1208 |
| CompleteZoneManager (all zones+links)  | 360041/29100 |  99952/ 1208 |
|----------------------------------------+--------------+--------------|
| Complete ZoneSorterByName [3]          | 271289/29100 |    752/    0 |
| Complete ZoneSorterByOffsetAndName [3] | 271337/29100 |    800/    0 |
+---------------------------------------------------------------------+

```

## ESP32

* ESP32-01 Dev Board, 240 MHz Tensilica LX6
* Arduino IDE 1.8.19, Arduino CLI 1.1.1
* ESP32 Boards 2.0.9

```
+----------------------------------------------------------------------+
| Functionality                          |  flash/  ram |        delta |
|----------------------------------------+--------------+--------------|
| baseline                               | 228345/21976 |      0/    0 |
|----------------------------------------+--------------+--------------|
| LocalDateTime                          | 230805/21984 |   2460/    8 |
| ZonedDateTime                          | 231785/22000 |   3440/   24 |
| Manual ZoneManager                     | 231797/21976 |   3452/    0 |
|----------------------------------------+--------------+--------------|
| Basic TimeZone (1 zone)                | 236409/22184 |   8064/  208 |
| Basic TimeZone (2 zones)               | 236845/22392 |   8500/  416 |
| BasicZoneManager (1 zone)              | 236561/22208 |   8216/  232 |
| BasicZoneManager (all zones)           | 252225/22208 |  23880/  232 |
| BasicZoneManager (all zones+links)     | 261121/22208 |  32776/  232 |
|----------------------------------------+--------------+--------------|
| Basic ZoneSorterByName [1]             | 237113/22208 |    552/    0 |
| Basic ZoneSorterByOffsetAndName [1]    | 237193/22208 |    632/    0 |
|----------------------------------------+--------------+--------------|
| Extended TimeZone (1 zone)             | 238521/22744 |  10176/  768 |
| Extended TimeZone (2 zones)            | 238941/23504 |  10596/ 1528 |
| ExtendedZoneManager (1 zone)           | 238657/22752 |  10312/  776 |
| ExtendedZoneManager (all zones)        | 269457/22752 |  41112/  776 |
| ExtendedZoneManager (all zones+links)  | 279393/22752 |  51048/  776 |
|----------------------------------------+--------------+--------------|
| Extended ZoneSorterByName [2]          | 239209/22752 |    552/    0 |
| Extended ZoneSorterByOffsetAndName [2] | 239285/22752 |    628/    0 |
|----------------------------------------+--------------+--------------|
| Complete TimeZone (1 zone)             | 238857/22744 |  10512/  768 |
| Complete TimeZone (2 zones)            | 240129/23504 |  11784/ 1528 |
| CompleteZoneManager (1 zone)           | 238993/22752 |  10648/  776 |
| CompleteZoneManager (all zones)        | 318513/22752 |  90168/  776 |
| CompleteZoneManager (all zones+links)  | 328465/22752 | 100120/  776 |
|----------------------------------------+--------------+--------------|
| Complete ZoneSorterByName [3]          | 239545/22752 |    552/    0 |
| Complete ZoneSorterByOffsetAndName [3] | 239617/22752 |    624/    0 |
+---------------------------------------------------------------------+

```

