AceTime 2.4.0 Date and time classes for Arduino that support timezones from the TZ Database.

compat.h
Go to the documentation of this file.
1 /*
2 * MIT License
3 * Copyright (c) 2018 Brian T. Park
4 */
5
6 #ifndef ACE_TIME_ZONEINFO_COMPAT_H
7 #define ACE_TIME_ZONEINFO_COMPAT_H
8
18 #include <stdint.h>
19 #include <string.h>
20 #include <WString.h> // FPSTR(), __FlashStringHelper
21
23 #define ACE_TIME_USE_PROGMEM 1
24 #if ACE_TIME_USE_PROGMEM
25 #define ACE_TIME_PROGMEM PROGMEM
26 #else
27 #define ACE_TIME_PROGMEM
28 #endif
29
30 // Some 3rd party Arduino cores does not define FPSTR(). And unfortunately, when
31 // they do, sometimes it's wrong, so we sometimes have to clobber it below.
32 #if ! defined(FPSTR)
33 #define FPSTR(p) (reinterpret_cast<const __FlashStringHelper *>(p))
34 #endif
35
36 // Include the correct pgmspace.h depending on architecture.
37 #if defined(ARDUINO_ARCH_AVR)
38 #include <avr/pgmspace.h>
39
40 // Seeeduino SAMD21 Core does not define an identifier for the following, so
41 // they are not supported:
42 // * Wio lite MG126
43 // * Wio GPS Board
44 // * Wio LTE CAT.1
45 //
46 #elif defined(SEEED_XIAO_M0) \
47 || defined(SEEEDUINO_ZERO) \
48 || defined(SEEED_FEMTO_M0) \
49 || defined(SEEEDUINO_LORAWAN) \
50 || defined(SEEED_WIO_TERMINAL) \
51 || defined(SEEED_GROVE_UI_WIRELESS)
52
53 #include <avr/pgmspace.h>
54
55 // Seeeduino (as of 1.8.3) provides an incorrect definition of FPSTR()
56 // so we have to clobber it.
57 #undef FPSTR
58 #define FPSTR(p) (reinterpret_cast<const __FlashStringHelper *>(p))
59
60 #elif defined(ARDUINO_ARCH_SAMD)
61 #include <avr/pgmspace.h>
62
63 // Set this to 1 to clobber SERIAL_PORT_MONITOR to SerialUSB on
64 // an original Arduino Zero when using the Native port. See USER_GUIDE.md for
65 // more info.
66 #define ACE_TIME_CLOBBER_SERIAL_PORT_MONITOR 0
67 #if ACE_TIME_CLOBBER_SERIAL_PORT_MONITOR && defined(ARDUINO_SAMD_ZERO)
68 #undef SERIAL_PORT_MONITOR
69 #define SERIAL_PORT_MONITOR SerialUSB
70 #endif
71
72 #elif defined(ARDUINO_ARCH_STM32)
73 #include <avr/pgmspace.h>
74
75 #elif defined(ARDUINO_ARCH_ESP8266)
76 #include <pgmspace.h>
77
78 #elif defined(ARDUINO_ARCH_ESP32)
79 #include <pgmspace.h>
80
81 #if ! defined(SERIAL_PORT_MONITOR)
82 #define SERIAL_PORT_MONITOR Serial
83 #endif
84
85 #elif defined(TEENSYDUINO)
86 #include <avr/pgmspace.h>
87
88 #elif defined(EPOXY_DUINO)
89 #include <pgmspace.h>
90
91 #else
92 #warning Untested platform. AceTime may still work...
93
94 #include <avr/pgmspace.h>
95
96 #endif
97
98 #endif // ACE_TIME_ZONEINFO_COMPAT_H