pfodParser 3.61.0 The pfodParser library is handles commands sent from the Android pfodApp, pfodApp supports WiFi, BLE, Bluetooth and SMS connections

pfodESPBufferedClient.h
Go to the documentation of this file.
1 #ifndef pfodESPBufferedClient_h
2 #define pfodESPBufferedClient_h
13 #if defined (ESP32) || defined (ESP8266) || defined (ARDUINO_SAMD_NANO_33_IOT)
14
15 #include "Stream.h"
16 #include "WiFiClient.h"
17 class pfodESPBufferedClient : public Stream {
18
19 public:
20 pfodESPBufferedClient(); // default 1460 byte buffer and default send delay 10mS
21 pfodESPBufferedClient* connect(WiFiClient* _client);
22 virtual size_t write(uint8_t);
23 virtual size_t write(const uint8_t *buf, size_t size);
24 virtual int available();
25 virtual int availableForWrite();
26 virtual int read();
27 virtual int peek();
28 virtual void flush();
29 virtual void stop();
30 virtual uint8_t connected();
31 void setDebugStream(Print* out);
32 private:
33 WiFiClient* client;
34 void sendAfterDelay();
35 void forceSend();
36 size_t _write(uint8_t c);
37 static const unsigned long DEFAULT_SEND_DELAY_TIME = 10; // 10mS delay before sending buffer
38 //#define WIFICLIENT_MAX_PACKET_SIZE 1460
39 static const size_t DEFAULT_SEND_BUFFER_SIZE = 1460; //WIFICLIENT_MAX_PACKET_SIZE; // Max data size for standard TCP/IP packet
40 // at 57600 baud can read about 1152 bytes in 0.2sec so limit serial to <=57600 to prevent losing data
41 uint8_t sendBuffer[DEFAULT_SEND_BUFFER_SIZE]; //
42 size_t sendBufferIdx = 0;
43 unsigned long sendTimerStart = 0;
44 unsigned long sendDelayTime;
45 Print* debugOut;
46 };
47
48 #endif
49
50 #endif // pfodESPBufferedClient_h