pfodParser 3.61.0 The pfodParser library is handles commands sent from the Android pfodApp, pfodApp supports WiFi, BLE, Bluetooth and SMS connections

pfodSMS_SIM5320.h
Go to the documentation of this file.
1 #ifndef pfodSMS_SIM5320_h
2 #define pfodSMS_SIM5320_h
3
4 /*
5 (c)2014-2018 Forward Computing and Control Pty. Ltd.
6 NSW Australia, www.forward.com.au
7 This code is not warranted to be fit for any purpose. You may only use it at your own risk.
8 This code may be freely used for both private and commercial use
9 Provide this copyright is maintained.
10 */
11 /*
12 This library uses about 22K of ROM (program space) and 3234 bytes of RAM
13 and so is NOT suitable for use on an UNO
14 Use a Mega2560 or similar with more then 4K of RAM
15 */
16
17 #include "Arduino.h"
18
19 #include "pfodStream.h"
20 #include "pfod_Base.h"
21 #include "pfod_rawOutput.h"
22
23 #define SMS_MAX_SIZE 160
24 #define SMS_RX_BUFFER_SIZE 267
25 // max msg size after decode 256 + + 8(hash) + 2(extra) +null
26 // max pfod msg size
27 #define SMS_TX_MSG_SIZE 1026
28 // 1024 + 2
29 #define SMS_TX_BUFFER_SIZE (SMS_TX_MSG_SIZE+8+2)
30 // add a little 1026 + 8(hash) + 2(extra) + null
31
32 class pfodSMS_SIM5320: public pfod_Base {
33
34 public:
35 pfodSMS_SIM5320();
36 void init(Stream *_gprs, int resetPin = -1, int powerOnOffPin = -1, int powerStatusPin = -1); // use -1 if not used
37 void setDebugStream(Stream* out);
38 unsigned long getDefaultTimeOut();
39 Print* getRawDataOutput();
40 int available(void);
41 int peek(void);
42 int read(void);
43 void flush(void);
44 size_t write(uint8_t);
45 size_t writeRawData(uint8_t c);
46 Stream* getPfodAppStream(); // use pfodSecurity.getPfodAppStream() instead get the command response stream we are reading from and writing to
47 void _closeCurrentConnection();
48
49
50 private:
51 int powerResetPin;
52 int powerStatusPin;
53 int resetPin;
54 const static int MAX_PHNO_LEN = 20;
55 const static int MAX_PHNO_CHECK = 6; // from end
56 struct connection {
57 int connectionNo; // = 0; is valid
58 int msgNo_rx; // = 0; // first expected
59 int msgNo_tx; // = 0; // next msgNo for next SMS being sent
60 int msgNo_tx_newMsg; // = 0; next msgNo for start of new response
61 // the msgNo_tx is set to this on a new msg
62 int msgNo_tx_resend; // = 0; // starting msgNo for last response
63 // the msgNo_tx is set to this on resend
64 boolean timedOut;
65 //knownConnection conPtr*;
66 char returnPhNo[MAX_PHNO_LEN + 1]; // plus null idx runs from 0 to MAX_PHNO_LEN
67 };
68
69 struct knownConnection {
70 int connectionNo; // = 0; is valid
71 char returnPhNo[MAX_PHNO_LEN + 1]; // plus null idx runs from 0 to MAX_PHNO_LEN
72 };
73
74 static const int MAX_KNOWN_CONNECTION = 10;
75 struct knownConnection knownConnectionsArray[MAX_KNOWN_CONNECTION]; // this allocate space for structs as well
76 struct knownConnection* knownArrayPtrs[MAX_KNOWN_CONNECTION]; // allocate space for ptrs
77
78 void init();
79 void initPowerUp();
80 int findEmptyKnownConnection();
81 void updateMsgNoForStartNewCommand();
82 void updateMsgNoForStartResend();
83
84 void stopResponseSends();
85 void stopAllSends();
86
87 void clearKnownConnection(knownConnection * kCon);
88 void clearKnownConnection(int idx);
89 void printKnownConnections();
90 void printKnownConnection(knownConnection * kCon);
91 void swapKnownConnections();
92 void setTopKnownConnectionFromCurrent();
93 void moveKnownConnectionToTop(int idx);
94 void updateKnownConnectionNo(connection * con); // always succeeds
95 void updateKnownConnectionNoAndMoveToTop(connection * con); // always succeeds
96 void setNextExpectedConnectionMsgNo(connection * con, boolean foundEndParens);
97
98 typedef enum decode_sms_return_t {
99 IGNORE, // invalid msg, wrong msgNo etc
100 RESEND_LAST_RESPONSE, // ignore msg and resend last response
101 CLOSE_CONNECTION, // close current connection no change in connectionNo
102 START_NEW_COMMAND, // start a new command no new connection
103 PROCESS_NEXT_PART_OF_COMMAND, // process continuation SMS of a command for connection expectedMsgNo has been updated
104 CLOSE_CONNECTION_AND_UPDATE_CONNECTION, // close current and update for new connectionNo
105 NEW_CONNECTION_SAME_PHONE_NO, // new connect but with same phoneNo
106 IGNORE_CONNECTION, // ignore connection attempt as current connection not timed out but let pfodApp retry
107 START_NEW_CONNECTION, // start a new connection from a different phone no
108 START_NEW_CONNECTION_AND_CLOSE // start new connection but msg is {!} so no reply but send alert to current and process msg
109 } decode_sms_return_t;
110
111 decode_sms_return_t decodeSMS(connection * current, connection * next, const char* smsChars, byte * decodedSMS,
112 size_t* currentDecodedLen);
113
114 bool havePowerResetPins;
115 bool haveResetPin;
116 void clearParser();
117 void clearResponseSet();
118 boolean decodeSMScmd(const char*smsChars, byte * decodedSMS, size_t* currentDecodedLen);
119 int checkSMSmsgForValidNewConnection(int connectionNo, int msgNo, const char* decodedSMS, boolean foundCmdClose);
120 size_t encodeSMS(int connectionNo, int msgNo, const byte * msgBytes, size_t msgBytesIdx, char* encodedSMS);
121 //boolean isResendStoredSMS();
122
123 const char* findStr(const char* msg, const __FlashStringHelper * ifsh);
124 const char *findStr(const char* str, const char* target);
125
126 const static size_t MAX_BYTES_TO_CONVERT = 117;
127
128 const static int MAX_MSG_NO_LEN = 3;
129 const static int MAX_MSG_LEN = 256; // max msg len then null
130 char gprsMsg[MAX_MSG_LEN + 1]; // plus null idx runs from 0 to MAX_MSG_LEN
131 int gprsMsgIdx; // = 0;
132 unsigned char gprsLastChar; // = '\0';
133 // keep track of the next 10 incoming SMS sim card msg numbers are reported by +CMTI:
134 const static int MAX_INCOMING_MSG_NOS = 10; // = 10+1 for head != tail
135
136 uint8_t incomingMsgNos_head; // from 0 to MAX_INCOMING_MSG_NOS;
137 uint8_t incomingMsgNos_tail; // from 0 to MAX_INCOMING_MSG_NOS;
138 // add to head take from tail
139 // stop adding when head+1%MAX_INCOMING_MSG_NOS+1 == tail
140 // stop taking when tail == head
141 // start tail==head == 0;
142 // take (tail == head) so empty
143 // add test (head+1%MAX_INCOMING_MSG_NOS != tail) add to [head] and head++
144 // take tail!= head take[tail++] now tail == head
145 // add 3 [0],[1]
146 char incomingMsgNos[MAX_INCOMING_MSG_NOS + 1][MAX_MSG_NO_LEN + 1];
147 void requestIncomingSmsMsg(const char *msgNo);
148
149 size_t rxBufferLen; // runs from 0 to SMS_RX_BUFFER_SIZE
150 size_t txBufferLen; // runs from 0 to SMS_TX_BUFFER_SIZE
151 size_t rxBufferIdx; // runs from 0 to rxBufferLen
152 size_t txBufferIdx; // runs from 0 to txBufferLen
153 byte rxBuffer[SMS_RX_BUFFER_SIZE + 1]; // allow for terminating null
154 byte txBuffer[SMS_TX_BUFFER_SIZE + 1]; // allow for terminating null
155 char responseSMSbuffer[SMS_MAX_SIZE + 1]; // only 160 + 1
156 static const int SMS_RAWDATA_TX_BUFFER_SIZE = MAX_BYTES_TO_CONVERT - 1; //117
157 byte rawdataTxBuffer[SMS_RAWDATA_TX_BUFFER_SIZE + 1]; // allow for terminating null and force null at end
158 size_t rawdataTxBufferLen; // runs from 0 to SMS_RAWDATA_TX_BUFFER_SIZE
159 size_t rawdataTxBufferIdx; // runs from 0 to rawdataTxBufferLen
160 char rawdataSMSbuffer[SMS_MAX_SIZE + 1]; // only 160 + 1
161 void flushRawData();
162 void clearRawdataTxBuffer();
163 boolean isSendingResponse();
164 boolean haveRequestedIncomingMsg;
165 void requestNextIncomingMsg();
166
167 boolean expectingMessageLines; // note msg from pfodApp may have embedded new line
168 boolean sendingRawdata; // true if processing and sending SMS response to command
169 boolean sendingResponse; // true if processing and sending SMS response to command
170 boolean sendingResend; // true if processing and sending SMS resend of previous response to command
171 boolean resendLastResponse; // true if should start resend of last response
172 // if sendingResponse then canSendRawData() return false and any write is just dropped
173 boolean responseSet; // true if tx_buffer holds respons upto } and no new cmd recieved
174 boolean deleteReadSmsMsgs; // true if should delete read msgs
175 boolean foundOK; // true when OK was last gprs msg
176
177 struct connection connection_A;
178 struct connection connection_B;
179 struct connection *currentConnection;
180 struct connection *nextConnection;
181 void pollSMSboard();
182 void sendSMSrawData();
183
184 const char* collectGprsMsgs();
185 void clearGprsLine();
186 void processGprsLine(const char* line);
187 // maxLen includes null at end
188 // void getProgStr(const __FlashStringHelper *ifsh, char*str, int maxLen);
189 int decodeInt(const char*smsChars, size_t idx);
190 size_t encodeInt(int number, char*rtn, size_t idx);
191 size_t convertThree8Bytes(long three8Bytes, char*rtn, size_t idx);
192 byte decodeSMSChar(byte encodedChar);
193 byte encodeSMSChar(byte encodedChar);
194 //Stream *console;
195 Stream *gprs; // sms shield serial connection
196 const static byte invalidSMSCharReturn = 0xff; // == 255,
197 byte bytesToConvert[MAX_BYTES_TO_CONVERT + 1]; // max bytes to convert + null
198
199 void closeConnection(connection * con);
200 void clearConnection(connection * con);
201
202 boolean newConnectionNumberGreater(int current, int next);
203 boolean validSMSmsgLen(const char* smsChars);
204 void printIgnoreOutOfSequence();
205 //unsigned long timedOutTimer;
206 //unsigned long start_mS;
207 int findMatchingKnownPhoneNo(const char *phNo);
208 boolean phoneNoMatchesCurrent(const char*newPhNo);
209 boolean phoneNoMatches(const char*oldPhNo, const char*newPhNo);
210 boolean phoneNoHas6Digits(const char *phNo);
211 void checkGPRSpoweredUp();
212 int powerCycleGPRS();
213 boolean setupSMS();
214 boolean gprsReady;
215 boolean powerUpGPRS();
216 void clearTxBuffer();
217
218 void printConnection(connection * con);
219 void swapConnections();
220 void setPhoneNo(connection * con, const char* phNo);
221
222 void printCurrentConnection();
223 void printNextConnection();
224 // void startTimer();
225
226 void startSMS(const char* phoneNo);
227 void sendNextSMS(); // send next part of txbuffer
228 void clearReadSmsMsgs();
229 void clearAllSmsMsgs();
230 bool clearAllSmsMsgsOnInit();
231 void emptyIncomingMsgNo();
232
233 void gprsPrint(const char* str);
234 void gprsPrint(char c);
235 void gprsPrint(const __FlashStringHelper * ifsh);
236
237 boolean haveIncomingMsgNo();
238 boolean addIncomingMsgNo(const char* msgNo);
239 const char* getIncomingMsgNo();
240 void deleteIncomingMsg(const char *newMsgNo);
241
242 void turnEchoOn();
243 void turnEchoOff();
244
245 pfod_rawOutput raw_io;
246 pfod_rawOutput* raw_io_ptr;
247
248
249 private:
250 Stream* debugOut;
251
252 };
253
254 #endif // pfodSMS_SIM5320_h
255
pfod_Base
pfod_Base for Arduino Base class for all pfod_Base_xxxx classes The subclasses pfod_Base_xxx must ove...
Definition: pfod_Base.h:18
pfod_rawOutput
Definition: pfod_rawOutput.h:15
pfodSMS_SIM5320
Definition: pfodSMS_SIM5320.h:32
pfodSMS_SIM5320::getRawDataOutput
Print * getRawDataOutput()
pfodSMS_SIM5320::write
size_t write(uint8_t)
pfodSMS_SIM5320::peek
int peek(void)
pfodSMS_SIM5320::pfodSMS_SIM5320
pfodSMS_SIM5320()
pfodSMS_SIM5320::getPfodAppStream
Stream * getPfodAppStream()
pfodSMS_SIM5320::init
void init(Stream *_gprs, int resetPin=-1, int powerOnOffPin=-1, int powerStatusPin=-1)
pfodSMS_SIM5320::getDefaultTimeOut
unsigned long getDefaultTimeOut()
pfodSMS_SIM5320::writeRawData
size_t writeRawData(uint8_t c)
pfodSMS_SIM5320::available
int available(void)
pfodSMS_SIM5320::read
int read(void)
pfodSMS_SIM5320::setDebugStream
void setDebugStream(Stream *out)
pfodSMS_SIM5320::_closeCurrentConnection
void _closeCurrentConnection()
pfodSMS_SIM5320::flush
void flush(void)
pfod_Base.h
pfod_rawOutput.h
SMS_TX_BUFFER_SIZE
#define SMS_TX_BUFFER_SIZE
Definition: pfodSMS_SIM5320.h:29
SMS_MAX_SIZE
#define SMS_MAX_SIZE
Definition: pfodSMS_SIM5320.h:23
SMS_RX_BUFFER_SIZE
#define SMS_RX_BUFFER_SIZE
Definition: pfodSMS_SIM5320.h:24
pfodStream.h