pfodParser 3.61.0 The pfodParser library is handles commands sent from the Android pfodApp, pfodApp supports WiFi, BLE, Bluetooth and SMS connections

Classes | Macros
pfodRawCmdParser.h File Reference
`#include "Arduino.h"`
`#include "pfodStream.h"`
`#include "pfodParser.h"`

Go to the source code of this file.

## Classes
class | pfodRawCmdParser

## Macros
#define | pfod_MAYBE_UNUSED(x) (void)(x)
| pfodRawCmdParser for Arduino Parses commands of the form { cmd | arg1 `arg2 ...` More...

## Macro Definition Documentation

## ◆ pfod_MAYBE_UNUSED

#define pfod_MAYBE_UNUSED | ( |  | x | ) | (void)(x)

pfodRawCmdParser for Arduino Parses commands of the form { cmd | arg1 `arg2 ...`

} Arguments are separated by The | and the args are optional This is a complete paser for ALL commands a pfodApp will send to a pfodDevice see www.pfod.com.au for more details.

pfodRawCmdParser adds about 482 bytes to the program and uses about 260 bytes RAM

The pfodRawCmdParser parses messages of the form { cmd | arg1 `arg2` ... } The message is parsed into the args array by replacing '|', '‘’ and '}' with '/0' (null) When the the end of message } is seen parse() returns the first byte of the cmd getCmd() returns a pointer to the null terminated cmd skipCmd() returns a pointer to the first arg (null terminated) or a pointer to null if there are no args getArgsCount() returns the number of args found. These calls are valid until the start of the next msg { is parsed. At which time they are reset to empty command and no args.

Definition at line 39 of file pfodRawCmdParser.h.