pfodParser 3.61.0 The pfodParser library is handles commands sent from the Android pfodApp, pfodApp supports WiFi, BLE, Bluetooth and SMS connections

pfodRadioMsg Member List

This is the complete list of members for pfodRadioMsg, including all inherited members.

ackedMsgSeqNo | pfodRadioMsg | protected
addressedTo | pfodRadioMsg | protected
BUFFER_SIZE | pfodRadioMsg | protected static
getAckedMsgSeqNo() | pfodRadioMsg |
getAddressedTo() | pfodRadioMsg |
getBuf() | pfodRadioMsg |
getLen() | pfodRadioMsg |
getMaxMsgBufferSize() | pfodRadioMsg |
getMsgSeqNo() | pfodRadioMsg |
getReceivedFrom() | pfodRadioMsg |
init(size_t _maxMsgLen) | pfodRadioMsg |
isAckFor(pfodRadioMsg *lastRadioMsg) | pfodRadioMsg |
isNewConnectionRequest(uint8_t ourAddress) | pfodRadioMsg |
isNewMsg(uint8_t _thisAddress, uint8_t _targetAddress, uint8_t _expectedMsgSeqNo, bool isServer) | pfodRadioMsg |
isPureAck() | pfodRadioMsg |
isPureAckFor(uint8_t msgSeqNoWaitingForAck) | pfodRadioMsg | protected
isResendRequest(pfodRadioMsg *lastRadioMsg) | pfodRadioMsg |
maxMsgLen | pfodRadioMsg | protected
msgBuf | pfodRadioMsg | protected
msgLen | pfodRadioMsg | protected
msgSeqNo | pfodRadioMsg | protected
pfodRadioMsg() | pfodRadioMsg |
receivedFrom | pfodRadioMsg | protected
saveMsg(uint8_t *_buf, uint8_t _len, uint8_t _addressedTo, uint8_t _receievedFrom, uint8_t _msgSeqNo, uint8_t _ackedMsgSeqNo) | pfodRadioMsg |
saveMsg(Stream *_txBufPtr, uint8_t _addressedTo, uint8_t _receievedFrom, uint8_t _msgSeqNo, uint8_t _ackedMsgSeqNo) | pfodRadioMsg |
setAckedMsgSeqNo(uint8_t _ackedMsgSeqNo) | pfodRadioMsg |