#

## pfodWeb Connection Setup

Loading...
(c)2025 https://www.forward.com.au/pfod/pfodWeb
Select Connection Protocol:
HTTP
Serial
BLE
Connection Protocol:
IP Address:
Enter the IP address and optional port (default: port 80)
Baud Rate:
Select baud rate, then click Connect to choose serial port
Click Connect to scan for BLE devices
Timeout (s):
Chart Only Mode -- Opens chart display directly instead of main menu