pfodParser 5.0.1 The pfodParser library is handles commands sent from the Android pfodApp, pfodApp supports WiFi, BLE, Bluetooth and SMS connections

pfodMACClient.h
Go to the documentation of this file.
1 #ifndef pfodMACClient_h
2 #define pfodMACClient_h
9 /*
10 * (c)2014-2017 Forward Computing and Control Pty. Ltd.
11 * NSW Australia, www.forward.com.au
12 * This code is not warranted to be fit for any purpose. You may only use it at your own risk.
13 * This code may be freely used for both private and commercial use
14 * Provide this copyright is maintained.
15 */
16
17 #include <Arduino.h>
18 #include "pfodStream.h"
19 #include "pfodMAC.h"
20
21 class pfodMACClient {
22 public:
23
24 pfodMACClient();
25 boolean init();
26
27
28 void setSecretKey(byte *key, int len);
29
30 void setDebugStream(Print* out);
31 boolean isValid(); // powercycles > 0
32 boolean isBigEndian(); // is 1 stored as 0x00000001 false for Atmel 8 bit micros
33
34
35
36 // useful for debugging
37 void printBytesInHex(Print *out, const byte* b, size_t len);
38
39
40 void initHash(); // start a new hash by initializing with the secret key
41 void putByteToHash(byte b); // add a byte to the hash
42 void putBytesToHash(byte* b, int len); // add a byte array to the hash
43 void putLongToHash(uint32_t l); // add a long to the hash (in BigEndian format)
44 void finishHash(); // finish the hash and calculate the result
45 byte* getHashedResult(); // get pointer to the 8 byte result
46
47
55 boolean checkMsgHash(const byte* msgHash, uint16_t len);
56
57 void reverseBytes(byte *b, int len); // swap from order of bytes upto len, converts between Endians, Big to Little, Little to Big
58
59 // const static uint8_t msgHashByteSize = 4; // number of byte in per msg hash
60 // const static uint8_t challengeHashByteSize = 8; // number of bytes in challenge hash
61 // const static uint8_t challengeByteSize = 8; // number of bytes in challenge
62 // const static uint8_t maxKeySize = 16; // max size of key 128 bits
63
64 unsigned char *hashChallenge(byte *challenge); // hashes challenge returns pointer to 8 byte result
65
66 private:
67 boolean initCalled; // set true after first init() call. Stops multiple calls to get readPowerCycles
68 boolean cmpToResult(const byte* response, uint16_t len);
69 Print *debugOut;
70 byte key[pfodMAC::maxKeySize]; // the secret key after reading from EEPROM and expanding to 16 bytes
71 uint8_t keyLen; // 0 if no key, else 16 (after padding key with 0 if shorter)
72 boolean bigEndian; // true if bigEndian uC
73
74 };
75
76
77 #endif // pfodMACClient_h
78
pfodMACClient
pfodMACClient for Arduino Updates power cycles, builds the Challenge, keeps track in message counts a...
Definition: pfodMACClient.h:21
pfodMACClient::isBigEndian
boolean isBigEndian()
pfodMACClient::printBytesInHex
void printBytesInHex(Print *out, const byte *b, size_t len)
pfodMACClient::setDebugStream
void setDebugStream(Print *out)
pfodMACClient::putByteToHash
void putByteToHash(byte b)
pfodMACClient::pfodMACClient
pfodMACClient()
pfodMACClient::getHashedResult
byte * getHashedResult()
pfodMACClient::finishHash
void finishHash()
pfodMACClient::reverseBytes
void reverseBytes(byte *b, int len)
pfodMACClient::setSecretKey
void setSecretKey(byte *key, int len)
pfodMACClient::isValid
boolean isValid()
pfodMACClient::putBytesToHash
void putBytesToHash(byte *b, int len)
pfodMACClient::hashChallenge
unsigned char * hashChallenge(byte *challenge)
pfodMACClient::putLongToHash
void putLongToHash(uint32_t l)
pfodMACClient::initHash
void initHash()
pfodMACClient::init
boolean init()
pfodMACClient::checkMsgHash
boolean checkMsgHash(const byte *msgHash, uint16_t len)
Converts msgHash from hex Digits to bytes and then compares the resulting byte[] with the current has...
pfodMAC::maxKeySize
static const uint8_t maxKeySize
Definition: pfodMAC.h:94
pfodMAC.h
pfodStream.h