pfodParser 5.0.1 The pfodParser library is handles commands sent from the Android pfodApp, pfodApp supports WiFi, BLE, Bluetooth and SMS connections

Class Hierarchy
This inheritance list is sorted roughly, but not completely, alphabetically:
[detail level 1 2 3]

C BufferRange | PfodCircularLineBuffer.h
▼C pfodAutoCmd |
C pfodDrawing |
C pfodControl |
C pfodDelay |
▼C pfodDwgsBase |
C pfodDwgs |
C pfodLinkedList< T > |
C pfodListNode< T > |
C pfodMAC |
C pfodMACClient | PfodMACClient for Arduino Updates power cycles, builds the Challenge, keeps track in message counts and hashes and check message hashes It uses upto 19 bytes of EEPROM starting from the address passed to init()
C pfodRadioDriver | PfodRadioDriver for Arduino This class abstracts the low level radio functions from pfodParser
C pfodRadioMsg | PfodRadioMsg for Arduino Holds a radio msg
C pfodWaitForUtils |
▼C Print |
▼C pfodParser |
C pfodSecurity |
C pfodRawDataWriter |
C pfod_rawOutput |
▼C Printable |
C pfodCmd |
C SipHash_2_4 |
▼C Stream |
C pfodBLEBufferedSerial | (c)2015 Forward Computing and Control Pty
C pfodBTCBufferedStream | (c)2015 Forward Computing and Control Pty
C pfodBufferedStream | (c)2018 Forward Computing and Control Pty
C pfodCircularLineBuffer | PfodCircularLineBuffer - Line-aware circular buffer for CSV data streaming
C pfodNonBlockingInput |
C pfodRawCmdParser |
C pfodRingBuffer | PfodRingBuffer for Arduino Implements a ring buffer implementation of an Arduino Stream upto 32K buffers NOTE: this implementation DOES NOT BLOCK if the buffer is full extra bytes written are quietly dropped
C pfodSecurityClient |
C pfodStreamString |
▼C pfod_Base | Pfod_Base for Arduino Base class for all pfod_Base_xxxx classes The subclasses pfod_Base_xxx must override all the methods below
C pfodRadio | An ack consists of a message with:
C pfodSMS_SIM5320 |
C pfodSMS_SIM900 |
▼C String |
C pfodStreamString |